SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_742083rv
	Type ( Engine )
	WagonShape ( cd_742083rv.s )
        FreightAnim ( cd_742083rvfg.s 0.1 0.1 )


	Comment ( ladenie OR )
	Comment ( svetla: Robo )
	Comment ( GC34P )	

comment	( Overall physics )


	Size ( 3.004m 4.439m 13.601m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 64.0t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.004m 4.439m 13.601m ) )

Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 0cm 0cm )
  )
  CouplingHasRigidConnection ( 1 )
  Velocity ( 0.01m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 0cm 0cm )
  )
  CouplingHasRigidConnection ( 1 )
  Velocity ( 0.01m/s )
 )

comment	( Adhesion and Friction )

	ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*64t )
	DerailBufferForce ( 800kN )
	NumWheels (	4 )
	Friction (
		923.9N/m/s    -0.10    1.5mph    11.731N/m/s    1.897
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)

	MaxBrakeForce( 84.18kN )
	MaxHandbrakeForce( 19.93kN )
	NumberOfHandbrakeLeverSteps( 10 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
        BrakeSystemType( "Air_single_pipe" )
        TripleValveRatio( 2.5 )
        MaxReleaseRate( 1.6 )
        MaxApplicationRate( 1.5 )
        MaxAuxilaryChargingRate( 4.28 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 52.50 )
        BrakePipeVolume ( 0.41 )
Comment (** Prubeh soucinitele treni dle rychlosti - litinove brzdove spalky **)

  	  ORTSBrakeShoeFriction (
  			0	0.31
			1	0.30
			2	0.28
			3	0.27
			4	0.26				
			5	0.25
			7	0.24
			8	0.23
			9	0.22
			12	0.21
			14	0.20
			17	0.19
			20	0.18
			24	0.17
			29	0.16
			34	0.15
			40	0.14
			47	0.13
			55	0.12
			66	0.11
			84	0.10
			115	0.09
			160	0.09
	)
	
comment	( EngSound, Freight, Inside, IntakePoint )

	Sound ( "../../common.snd/snd742/742gceng.sms" )
    	
	IntakePoint ( 0 2 FuelDiesel )

comment	( Lights )

	Lights ( 25
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFffff )
					Position ( 0 3.8 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0 3.8 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( -0.1 3.87 6.03 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.1 3.87 6.03 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( Tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.0 3.76 6.03 )
					Azimuth ( 0.0 0.0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
                 Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.705 2.088 6.05 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.705 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.705 1.84 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.705 1.84 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )
                Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.1 3.87 -6.03 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( -0.1 3.87 -6.03 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		
                Light (
			comment ( Tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.0 3.76 -6.03 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.705 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.705 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.705 1.84 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.705 1.84 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.705 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.705 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Pravé pYední pozi
ní - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.705 2.088 6.05 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light	(
			comment( Levé zadní pozi
ní - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.705 2.088 -6.05 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.705 2.088 6.05 )
					Azimuth ( 0 -5 5 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.705 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( Tretie svetlo )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.0 3.76 6.03 )
					Azimuth ( 0.0 0.0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.705 1.84 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.705 1.84 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
)


Engine ( cd_742083rv
ORTSDieselEngines ( 1
                Diesel (
                        IdleRPM ( 400 )
                        MaxRPM ( 1250 )
                        StartingRPM ( 380 )
                        StartingConfirmRPM ( 401 )
                        ChangeUpRPMpS ( 58 )
                        ChangeDownRPMpS ( 46 )
                        RateOfChangeUpRPMpSS ( 100 )
                        RateOfChangeDownRPMpSS ( 100 )
                        MaximalPower ( 780kW )
                        IdleExhaust ( 0.12 )
                        MaxExhaust ( 2.15 )
                        ExhaustDynamics ( 1.6 )
                        ExhaustColor ( 4O82DFFF )
                        ExhaustTransientColor ( 90FF00FF )
                        DieselPowerTab (
                                0  0
                                400  0
                                404  25000
                                450  50000
				500  100000
				650  234000
			        800  375000
			        980  510000
			       1100  645000
			       1250  780000
                        )
                        DieselConsumptionTab (
                                0  0
                                400  8.0
                                1250  220
                        ) 
                        ThrottleRPMTab (
                                0   400
                                3   404
                                6   450
                                13  500
                                30  650
                                48  800
                                65  980
                                83  1100
                                100 1250
                        )
                        DieselTorqueTab (
                                0  0
                                400  358.13
                                404  590.97
                                450  1061.11
				500  1910
				650  3438
			        800  4476.56
			        980  4969.9
			       1100  5599.77
			       1250  5959.2
                        )
                        MinOilPressure ( 36.20 )
                        MaxOilPressure ( 88 )
                        MaxTemperature ( 115 )
                        Cooling ( 3 )
                        TempTimeConstant ( 480 )
                        OptTemperature ( 85 )
                        IdleTemperature ( 42 )
                )
        )
	Wagon ( cd_742083rv )

	
comment	( Basic physical engine data )

	Type ( Diesel )
	MaxPower ( 780kW )
	MaxForce ( 192kN )	
	MaxContinuousForce ( 121kN )
	MaxCurrent ( 1200A ) 
	MaxVelocity ( 90km/h )
	DieselEngineSpeedOfMaxTractiveEffort( 21km/h )
	WheelRadius ( 0.5m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 21km/h )
	NumWheels ( 4 )
	
	
comment	( CabSound and Views )

	Sound ( "../../common.snd/snd742/742gccab.sms" )
 	
 	CabView ( "../../common.cab/cab742/742rvgc.cvf" )

	HeadOut ( 1.7 3.0 3.37 )
	DieselEngineType ( electric )
	MaxDieselLevel ( 1057gal )

comment	( Smoke and Steam )

	 Effects
	  (
	  DieselSpecialEffects
	   (
	    comment
	    (
	     the format of these little blocks is as follow:

	     offset.x offset.y offset.z
	     normal.x normal.y normal.z
	     width in metres

	     defining the offset from the shape pivot point
	     where steam / smoke should appear, the direction
	     it should go and the width of the nozzle
	    )

	    Exhaust1
	    (
	     0.0 4.6 1.25
	     0 1 0
	     0.1
	    )
	   )
         )

comment	( Brakes )


	AirBrakesAirCompressorPowerRating ( 2.55 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 145 )	
	AirBrakesMainResVolume ( 35.315 )
	AirBrakesAirCompressorWattage ( 20474 )
	AirBrakesCompressorRestartPressure ( 120 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 4.818 )
TrainBrakesControllerMaxApplicationRate ( 1.07 )
TrainBrakesControllerMaxReleaseRate ( 1.07 )
TrainBrakesControllerMaxQuickReleaseRate ( 2.14 )
TrainBrakesControllerEmergencyApplicationRate ( 5 )
TrainBrakesControllerMinSystemPressure ( 3 )
TrainBrakesControllerMaxSystemPressure ( 73 )
TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
TrainBrakesControllerMaxPressureDropInNormalApplication ( 29.2 )
TrainPipeLeakRate ( 0.033 )
TrainBrakesControllerFullServicePressureDrop ( 29.2 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

comment ( Monitors )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 58.9 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 59.0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)

EngineVariables( 1000 )

comment	( Controllers )

        EngineControllers (
		Throttle ( 0 1 0.125 0
			NumNotches ( 9
				Notch ( 0    0 Dummy )
				Notch ( 0.03 0 Dummy )
				Notch ( 0.06 0 Dummy )
				Notch ( 0.13 0 Dummy )
				Notch ( 0.30 0 Dummy )
				Notch ( 0.48 0 Dummy )
				Notch ( 0.65 0 Dummy )
				Notch ( 0.83 0 Dummy )
				Notch ( 1    0 Dummy )
			)
		)            
		comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 1 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
            comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 6
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	ORTSTractionCharacteristics (	10	10												
	throttle (	0	0.03	0.06	0.13	  0.30	  0.48	     0.65	 0.83	    1.00  )			
	table (													
		0km/h	0kN	12kN	19kN	44kN	 134kN	 192kN	    188kN	189kN	    192kN
               10km/h	0kN	8.00kN	12.60kN	29.40kN	73.08kN	 110.93kN   122.35kN	166.28kN    170.00kN
               20km/h	0kN	3.20kN	7.80kN	18.90kN	43.85kN	 66.13kN    79.53kN	100.78kN    115.00kN
               30km/h	0kN	2.40kN	4.80kN	13.30kN	29.23kN	 44.80kN    54.04kN	68.53kN	     82.00kN
               40km/h	0kN	1.60kN	4.20kN	9.80kN	22.41kN	 33.07kN    41.80kN	51.40kN	     60.00kN
               50km/h	0kN	0.80kN	3.00kN	7.70kN	17.54kN	 26.67kN    33.65kN	41.32kN	     50.00kN
               60km/h	0kN	0.00kN	2.40kN	7.00kN	15.59kN	 21.33kN    28.55kN	34.26kN	     43.00kN
               70km/h	0kN	0.00kN	1.80kN	6.30kN	13.64kN	 18.13kN    23.45kN	28.22kN	     35.00kN
               80km/h	0kN	0.00kN	1.20kN	4.90kN	10.72kN	 16.00kN    18.35kN	23.18kN	     28.00kN
               90km/h	0kN	0.00kN	0.60kN	4.20kN	9.74kN	 13.87kN    16.31kN	18.14kN	     23.00kN

		
		)													
	)
	
Comment	( Operations )


    	Name ( "CD 742.083-9 otocena" )
    	Description (
	 "Rada 742 CD je univerzalni dieselelektricka kapotova lokomotiva"+
	 "pro pouziti od posunovaciho provozu pres tazeni osobnich"+
	 "az do tazeni stredne tezkych nakladnich vlaku v dvojclennem rizeni.\n\n"+
	 "Usporadani dvojkoli: B0'B0'\n\n"+
	 "Prenos vykonu: elektricky\n\n"+
	 "Zdroj vykonu: naftovy motor CKD K 6 S 230 DR\n\n"+
	 "Vykon spalovaciho motoru: 883kW\n\n"+
	 "Max. provozni rychlost:  90km/h\n\n"+
	 "Trvala tazna sila na haku: 121kN pri 1200A\n\n"+
	 "Max. vyska: 4722mm\n\n"+
	 "Delka pres nar.: 13600mm\n\n"+
	 "Max. sirka: 3060mm\n\n"+
	 "Hmotnost plne vyzbroj. lokomotivy: 64t"  
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
		"4.	Stisknete D pro zvýsení pozadovaného výkonu.\n"+
		"5.	Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jedním stiskem ' presunte vlakovou brzdu do polohy ZÁVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
		"Jak pouzít vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
		"2.	Po dosazení pozadovaného brzdného tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
		"2.	Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
		"3.	Po odbrzdení a uvedení vlaku do pohybu stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n\n"+
 		"Jak pouzít lokomotvní brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivní brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0%).\n\n"+
		"Jak pouzít záchrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snízení výkonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
		"Jak zrusit záchrannou brzdu\n"+
		"1.	Pockejte na úplné zastavení vlaku.\n"+
		"2.	Stisknete Z pro odblokování ovládání lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
		"4.	Pomalu zvysujte výkon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Výstup a nástup cestujících\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahájení výstupu a nástupu cestujících.\n"+
		"3.	Pockejte na signál k odjezdu.\n"+
		"TIP: Pro zobrazení casu príjezdu a odjezdu u této a následující stanice pouzijte klávesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimální rychlost 1 km/h).\n"+
		"Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
		"2.	Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdíte pripojené vozy.\n\n"+
		"Odpojení vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftového stojanu stredem nádrze.\n"+
		"2.	Stisknete klávesu T a drzte ji po dobu doplnování nafty stisknutou.\n"+
		"TIP: Pro zobrazení prubehu plnení nádrze stisknete F9 a klepnete mysí na ikonu lokomotivy.\n\n"+
	)
)