SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cdc_742185

	Comment (** regulator GC34P **)
	Comment (** ladeni ORTS-MG s upravou vzduchariny. Autor upravy: Icik **)
	comment (** unor 2022 - Igor Hnizdo - uprava pro verzi ORCZ v1.6 **)

	Type ( Engine )
	WagonShape ( cdc_742185rv.s )
	ORTSFreightAnims (
        	 MSTSFreightAnimEnabled ( 0 )
		 	FreightAnimStatic (
		 	SubType( Default )
		 	Shape( "cdc_742185rvfg.s" )
		 	Offset( -0.0, 0.0, 0.0 )
		 	Visibility ( "Cab2D" )
		 	)
	)
	
Mass ( 64t )

Include 	("../common.eng/74x/udaje_742.inc")
Include 	("../common.inc/spriahlo/1-5cm.inc")
Include 	("../common.eng/74x/adheze_odpor_742.inc")
Include 	("../common.eng/74x/brzda_74x.inc")
comment (** unik vzduchu netesnosti brzdoveho potrubi **)
TrainPipeLeakRate ( 0.00258bar/s )
Include 	("../common.eng/74x/MBF_742.inc")
comment (** krivka soucinitele treni brzdovych zdrzi **)
Include 	("../common.inc/brzdna_krivka/zdrze-litina-PG.inc")
Include 	("../common.eng/74x/svetla_74x.inc")

comment (** smerovani na vnejsi ozvuceni **)
Sound ( "../../common.snd/snd742.159/742.159eng_IH_ORCZ.sms" )

     )

Engine ( cdc_742185

        Wagon ( cdc_742185 )

comment (** smerovani na pohled z kabiny **)
CabView ( "../../common.cab/cab742d/cab742d.cvf" )

comment (** smerovani na ozvuceni pohledu z kabiny **)
Sound ( "../../common.snd/snd742.159/742.159cab_IH_ORCZ.sms" )

Include 	("../common.eng/74x/HeadOut74x-rv.inc")
Include 	("../common.eng/74x/parametry_742GC34P.inc")
Include 	("../common.eng/74x/motor_K6S230-GC34P.inc")
Include 	("../common.eng/74x/efekty_kour_74xrv.inc")
Include 	("../common.eng/74x/tch742.inc")
Include 	("../common.eng/74x/vzduchotechnika_74x.inc")
Include 	("../common.inc/brzdice/BP-4bar.inc")
Include 	("../common.inc/brzdice/BS2.inc")
Include 	("../common.inc/MIREL_VZ/LS90_140kmh.inc")
Include 	("../common.eng/74x/ovladani_742.inc")


comment (** nazev v menu ORTS **)
Name ( "CDC 742.185-2 otocena" )

Description (
	 "Rada 742 CD je univerzalni dieselelektricka kapotova lokomotiva"+
	 "pro pouziti od posunovaciho provozu pres tazeni osobnich"+
	 "az do tazeni stredne tezkych nakladnich vlaku v dvojclennem rizeni.\n\n"+
	 "Usporadani dvojkoli: B0'B0'\n\n"+
	 "Prenos vykonu: elektricky\n\n"+
	 "Zdroj vykonu: naftovy motor CKD K 6 S 230 DR\n\n"+
	 "Vykon spalovaciho motoru: 883kW\n\n"+
	 "Max. provozni rychlost:  90km/h\n\n"+
	 "Trvala tazna sila na haku: 121kN pri 1200A\n\n"+
	 "Max. vyska: 4722mm\n\n"+
	 "Delka pres nar.: 13600mm\n\n"+
	 "Max. sirka: 3060mm\n\n"+
	 "Hmotnost plne vyzbroj. lokomotivy: 64t"  
    	)

)