SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( zscs_240082
	Type ( Engine )
	WagonShape ( zscs_240082.s )
        ORTSFreightAnims (
MSTSFreightAnimEnabled ( 0 )
FreightAnimStatic (
Shape ( zscs_240082fa.s )
Offset ( 0.0 0.0 0.0 )
Visibility ( "Outside" )
)
FreightAnimStatic (
Shape ( zscs_240082_2.s )
Offset ( 0.0 0.0 0.0 )
Flip ( 180 )
)
)

	Comment ( Eng created by ZSR - http://csd.webzdarma.cz )
	Comment ( Datum: 19/12/2008 )
	Comment ( Version: 1.07 )
	Comment ( Svetla: Robo )
  Comment	( 7/2020 - doplneni trakcni charakteristiky, uprava trakce a size: Acatus )
	Comment ( 7/2020 uprava vzduch brzd - klon z rady 242 od Josefa Vogeltanze )
	

comment	( Overall physics )

	Mass ( 84.5t )
	Size  ( 3.03m 4.55m 16.485m )
	CentreOfGravity ( 0m 2.25m 0m )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3.03m 4.55m 16.265m ) )	

comment	( Coupling )

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 850kN 850kN ) r0 ( 0cm 1.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness (  6.7e6N/m 4.4e8N/m) Break ( 850kN 850kN ) r0 ( 0cm 1.5cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )


Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.: 52t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 159kN )
MaxHandbrakeForce ( 51kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.212bar/s )
MaxApplicationRate ( 0.475bar/s )
MaxAuxilaryChargingRate ( 0.506bar/s )
EmergencyResChargingRate ( 0.506bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 4bar )
EmergencyResVolumeMultiplier ( 1.0 )
EmergencyResCapacity ( 240l )
BrakePipeVolume ( 14.4l )

ORTSBrakeShoeFriction ( 0 0.31 1 0.30 2 0.28 3 0.27 4 0.26 5 0.25 7 0.24 8 0.23 9 0.22 12 0.21 14 0.20 17 0.19 20 0.18 24 0.17 29 0.16 34 0.15 40 0.14 47 0.13 55 0.12 66 0.11 84 0.10 115 0.09 160 0.09 )


Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.3m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 2m 800mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Roller )
ORTSDavis_A ( 1051.3 )
ORTSDavis_B ( 27.64 )
ORTSDavis_C ( 6.0375 )

ORTSAdhesion (
ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
ORTSSlipWarningThreshold ( 70 )
)
   	
Comment (** Sberace - "delay" udava dobu zdvihani sberace, jelikoz simulator nedokaze identifikovat delku trvani animace sberace **)

ORTSPantographs (
Pantograph ( Delay ( 4s ) ) 
Pantograph ( Delay ( 4s ) ) 
 )
    
comment	( Freight, Inside, IntakePoint )
 	
	Inside (
		PassengerCabinFile ( zscs_240082.s )
		PassengerCabinHeadPos ( -1.7 3.2 5.7 )
		RotationLimit ( 45 100 0 )
		StartDirection ( 0 -90 0 )
	)

comment	( Lights )
comment ( svetelne kuzely ) 
	
	Lights ( 32
		Light (
			comment ( Svetelny kuzel dálkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0 1 8 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.09 3.8 7.48 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.09 3.8 7.48 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
                Light (
			comment ( reflektor tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 4.0 7.52 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 7.54 )
					Azimuth ( -15 -15 -15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.77 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.77 1.690 -7.5 )
					Azimuth ( 165 165 165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		
		comment ( Definicia svetiel pre zadne stanoviste )

		Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.09 3.8 -7.48 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.09 3.8 -7.48 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 7 7 7 )
				)
			)
		)
                Light (
			comment ( reflektor tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 4.0 -7.52 )
					Azimuth ( 180 180 180 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 -7.5 )
					Azimuth ( 165 165 165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadne lave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.77 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadne prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.77 1.690 7.5 )
					Azimuth ( -15 -15 -15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
                comment ( Definicia svetiel pre podvozky )
                Light (
			comment ( Prave predne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 4.854 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave predne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 4.854 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                Light (
			comment ( Prave zadne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 -4.854 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave zadne Vo)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 -4.854 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)    
                Light (
			comment ( Prave predne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 2.915 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave predne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 2.915 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                Light (
			comment ( Prave zadne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 1.40 0.772 -2.915 )
					Azimuth ( 0 0 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		) 
                Light (
			comment ( Lave zadne Vn)
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -1.40 0.772 -2.915 )
					Azimuth ( 0 -180 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)   
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( zadne leve pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		
		
		comment ( Definicia svetiel pre Loose consist )

		Light	(
			comment( Prave predne pozicne - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light	(
			comment( Lave zadne pozicne - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		

		comment ( Definicia svetiel pre HDV ovladane PC )

		Light (
			comment ( PC predne prave )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( 0.67 1.690 7.5 )
					Azimuth ( 15 15 15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( PC predne leve )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D  )
					Position ( -0.67 1.690 7.5 )
					Azimuth ( -15 -15 -15 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( reflektor tretie svetlo )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 4.0 7.52 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
		Light (
			comment ( PC zadne lave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.77 1.690 -7.5 )
					Azimuth ( -165 -165 -165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
		Light (
			comment ( PC zadne prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.77 1.690 -7.5 )
					Azimuth ( 165 165 165 )
					Transition ( 0 )
					Radius ( 0.5 )
				        Elevation ( 10 10 10 )
				)
			)
		)
	)
comment	( EngSound )

	Sound ( "..\\..\\common.snd\\sndelok\\240eng.sms" )


)

Engine ( zscs_240082  

comment	( Description )

	Wagon ( zscs_240082 )

	
comment	( Basic physical engine data )

	Type ( Electric )
	MaxPower ( 3200kW )
	MaxForce ( 183kN )	
	MaxContinuousForce ( 175kN )
	MaxCurrent ( 1083A )
	MaxVelocity ( 120kmh )
	DieselEngineSpeedOfMaxTractiveEffort( 0mph )  
	WheelRadius ( 0.625m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 90km/h )
	NumWheels ( 4 )
  ORTSDriveWheelWeight ( 84t )
  
   ORTSCruiseControl (
      Equipped ( True )
      MaxForceSteps ( 12 )
      AntiWheelSpinEquipped ( True )
      NominalSpeedStep ( 5 )
      DynamicBrakeMaxForceAtSelectorStep ( 7 ) 
      DynamicBrakeDescentCoefficient ( 0.5 )
      UseThrottle ( False )
      Options ( "RegulatorManual, RegulatorAuto, RegulatorTest, SelectorParking, SelectorNeutral, SelectorOn, SelectorStart" )
        )
        
        comment (** Hlavni vypinac **)

        ORTSCircuitBreaker ( Manual )
        ORTSCircuitBreakerClosingDelay ( 2s )
        ORTSPowerOnDelay ( 4s )

   comment ( 0     1     1     2     2     3     3     4     4     5     5     6     6     7     7     8     8     9     9    10    10    11    11    12    12    13    13    14    14    15    15    16    16    17    17    18    18    19    19    20    20    21    21    22    22    23    23    24    24    25    25    26    26    27    27    28    28    29    29    30    30    31    31    32    32    SI   SII  SIII  SIV ) 
ORTSContinuousForceTimeFactor ( 3600 )
ORTSTractionCharacteristics ( 25 70
Throttle ( 0.0   0.01  0.011 0.02 0.021 0.025 0.026  0.03 0.031  0.04 0.041  0.05 0.051  0.08 0.081  0.1  0.101  0.12 0.121  0.14 0.141  0.16 0.161  0.19 0.191  0.21 0.211  0.24 0.241  0.26 0.261  0.29 0.291  0.32 0.321  0.35 0.351  0.37 0.371  0.40 0.401  0.43 0.431  0.46 0.461  0.48 0.481  0.51 0.511  0.54 0.541  0.58 0.581  0.61 0.611  0.64 0.641  0.67 0.671  0.70 0.701  0.73 0.731  0.75 0.751  0.81  0.86  0.92  1 ) 
 table ( 
  0.0km/h 0.0kN  41kN  41kN  73kN  73kN 100kN 100kN 145kN 145kN 189kN 189kN 233kN 233kN 320kN 320kN 460kN 460kN 530kN 530kN 600kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN
  5.0km/h 0.0kN  21kN  21kN  36kN  36kN  54kN  54kN  79kN  79kN 108kN 108kN 138kN 138kN 175kN 175kN 212kN 212kN 250kN 250kN 310kN 310kN 400kN 400kN 550kN 550kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 10.0km/h 0.0kN  15kN  15kN  18kN  18kN  30kN  30kN  50kN  50kN  63kN  63kN  80kN  80kN 100kN 100kN 120kN 120kN 155kN 155kN 190kN 190kN 215kN 215kN 240kN 240kN 300kN 300kN 420kN 420kN 600kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 15.0km/h 0.0kN   9kN   9kN  10kN  10kN  15kN  15kN  28kN  28kN  39kN  39kN  49kN  49kN  60kN  60kN  72kN  72kN  85kN  85kN 103kN 103kN 133kN 133kN 163kN 163kN 191kN 191kN 220kN 220kN 280kN 280kN 350kN 350kN 450kN 450kN 570kN 570kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 20.0km/h 0.0kN   8kN   8kN   9kN   9kN  11kN  11kN  15kN  15kN  22kN  22kN  32kN  32kN  42kN  42kN  52kN  52kN  62kN  62kN  72kN  72kN  87kN  87kN 103kN 103kN 124kN 124kN 145kN 145kN 172kN 172kN 200kN 200kN 240kN 240kN 300kN 300kN 380kN 380kN 450kN 450kN 520kN 520kN 600kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 25.0km/h 0.0kN   7kN   7kN   8kN   8kN  10kN  10kN  14kN  14kN  20kN  20kN  23kN  23kN  28kN  28kN  37kN  37kN  45kN  45kN  53kN  53kN  63kN  63kN  73kN  73kN  85kN  85kN  98kN  98kN 114kN 114kN 130kN 130kN 162kN 162kN 193kN 193kN 230kN 230kN 300kN 300kN 380kN 380kN 450kN 450kN 540kN 540kN 600kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 30.0km/h 0.0kN   6kN   6kN   7kN   7kN   9kN   9kN  11kN  11kN  17kN  17kN  20kN  20kN  22kN  22kN  26kN  26kN  33kN  33kN  40kN  40kN  48kN  48kN  55kN  55kN  64kN  64kN  73kN  73kN  84kN  84kN  95kN  95kN 114kN 114kN 132kN 132kN 151kN 163kN 163kN 194kN 238kN 238kN 290kN 290kN 360kN 360kN 450kN 450kN 590kN 590kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 35.0km/h 0.0kN   5kN   5kN   6kN   6kN   8kN   8kN  10kN  10kN  15kN  15kN  19kN  19kN  20kN  20kN  22kN  22kN  25kN  25kN  32kN  32kN  37kN  37kN  42kN  42kN  49kN  49kN  58kN  58kN  66kN  66kN  74kN  74kN  86kN  86kN  98kN  98kN 119kN 119kN 140kN 140kN 165kN 165kN 191kN 191kN 230kN 230kN 275kN 275kN 350kN 350kN 420kN 420kN 500kN 500kN 600kN 600kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 40.0km/h 0.0kN   3kN   3kN   4kN   4kN   5kN   5kN   9kN   9kN  13kN  13kN  18kN  18kN  19kN  19kN  20kN  20kN  22kN  22kN  25kN  25kN  30kN  30kN  35kN  35kN  40kN  40kN  45kN  45kN  52kN  52kN  58kN  58kN  67kN  67kN  76kN  76kN  92kN  92kN 107kN 107kN 124kN 124kN 140kN 140kN 170kN 170kN 200kN 200kN 230kN 230kN 270kN 270kN 340kN 340kN 430kN 430kN 550kN 550kN 680kN 680kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN 700kN  
 45.0km/h 0.0kN   2kN   2kN   3kN   3kN   4kN   4kN   7kN   7kN  11kN  11kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  22kN  22kN  25kN  25kN  30kN  30kN  35kN  35kN  41kN  41kN  44kN  44kN  47kN  47kN  54kN  54kN  61kN  61kN  71kN  71kN  82kN  82kN  93kN  93kN 104kN 104kN 126kN 126kN 149kN 149kN 175kN 175kN 200kN 200kN 230kN 230kN 280kN 280kN 350kN 350kN 450kN 450kN 580kN 580kN 700kN 700kN 700kN 700kN 700kN 700kN  
 50.0km/h 0.0kN   2kN   2kN   2kN   2kN   3kN   3kN   5kN   5kN   9kN   9kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  23kN  23kN  28kN  28kN  31kN  31kN  35kN  35kN  40kN  40kN  44kN  44kN  47kN  47kN  50kN  50kN  60kN  60kN  67kN  67kN  75kN  75kN  83kN  83kN  98kN  98kN 114kN 114kN 136kN 136kN 158kN 158kN 183kN 183kN 208kN 208kN 250kN 250kN 320kN 320kN 420kN 420kN 550kN 550kN 700kN 700kN 700kN 700kN  
 55.0km/h 0.0kN   2kN   2kN   2kN   2kN   3kN   3kN   4kN   4kN   8kN   8kN  15kN  15kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  19kN  22kN  22kN  25kN  25kN  29kN  29kN  32kN  32kN  35kN  35kN  37kN  37kN  39kN  39kN  42kN  42kN  47kN  47kN  55kN  55kN  61kN  61kN  67kN  67kN  79kN  79kN  90kN  90kN 105kN 105kN 120kN 120kN 141kN 141kN 162kN 162kN 186kN 186kN 210kN 210kN 250kN 250kN 310kN 310kN 400kN 400kN 500kN 500kN  
 60.0km/h 0.0kN   2kN   2kN   2kN   2kN   2kN   2kN   4kN   4kN   7kN   7kN  14kN  14kN  15kN  15kN  16kN  16kN  17kN  17kN  18kN  18kN  21kN  21kN  22kN  22kN  23kN  23kN  26kN  26kN  29kN  29kN  32kN  32kN  35kN  35kN  37kN  37kN  45kN  45kN  52kN  52kN  55kN  55kN  59kN  59kN  65kN  65kN  73kN  73kN  85kN  85kN  99kN  99kN 115kN 115kN 131kN 131kN 152kN 152kN 174kN 174kN 195kN 195kN 212kN 212kN 256kN 256kN 300kN 300kN  
 65.0km/h 0.0kN   1kN   1kN   2kN   2kN   2kN   2kN   4kN   4kN   6kN   6kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  17kN  17kN  20kN  20kN  21kN  21kN  22kN  22kN  23kN  22kN  25kN  25kN  27kN  27kN  30kN  30kN  32kN  32kN  36kN  36kN  41kN  41kN  46kN  46kN  51kN  51kN  56kN  56kN  62kN  62kN  71kN  71kN  80kN  80kN  93kN  93kN 106kN 106kN 123kN 123kN 140kN 140kN 158kN 158kN 176kN 176kN 207kN 233kN 260kN 290kN  
 70.0km/h 0.0kN   1kN   1kN   2kN   2kN   2kN   2kN   4kN   4kN   5kN   5kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  19kN  19kN  20kN  20kN  21kN  21kN  22kN  22kN  23kN  23kN  24kN  24kN  26kN  26kN  28kN  28kN  31kN  31kN  35kN  35kN  39kN  39kN  44kN  44kN  49kN  49kN  54kN  54kN  61kN  61kN  68kN  68kN  77kN  77kN  88kN  88kN 102kN 102kN 116kN 116kN 130kN 130kN 147kN 147kN 179kN 203kN 225kN 241kN  
 75.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   4kN   4kN   4kN   4kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  18kN  18kN  19kN  19kN  20kN  20kN  21kN  21kN  23kN  23kN  24kN  24kN  25kN  25kN  25kN  25kN  27kN  27kN  31kN  31kN  35kN  35kN  38kN  38kN  43kN  43kN  47kN  47kN  53kN  53kN  59kN  59kN  66kN  66kN  73kN  73kN  83kN  83kN  93kN  93kN 105kN 105kN 119kN 119kN 149kN 171kN 185kN 203kN  
 80.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   4kN   4kN   4kN   4kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  22kN  22kN  23kN  23kN  24kN  24kN  24kN  24kN  25kN  25kN  27kN  27kN  31kN  31kN  35kN  35kN  38kN  38kN  43kN  43kN  48kN  48kN  52kN  52kN  58kN  58kN  63kN  63kN  71kN  71kN  80kN  80kN  90kN  90kN 100kN 100kN 127kN 147kN 161kN 176kN  
 85.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   3kN   2kN   4kN   4kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  19kN  14kN  21kN  21kN  22kN  23kN  23kN  23kN  23kN  24kN  24kN  25kN  25kN  27kN  27kN  31kN  31kN  34kN  34kN  37kN  37kN  42kN  42kN  45kN  45kN  50kN  50kN  55kN  55kN  63kN  63kN  68kN  68kN  77kN  77kN  85kN  85kN 108kN 127kN 140kN 154kN   
 90.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   3kN   3kN   4kN   4kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  15kN  15kN  16kN  16kN  17kN  17kN  18kN  18kN  20kN  20kN  20kN  20kN  21kN  21kN  22kN  22kN  23kN  23kN  24kN  24kN  26kN  26kN  29kN  29kN  33kN  33kN  36kN  36kN  39kN  39kN  41kN  41kN  45kN  45kN  49kN  49kN  54kN  54kN  59kN  59kN  67kN  67kN  74kN  74kN  93kN 109kN 122kN 133kN  
 95.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   3kN   3kN   8kN   8kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  14kN  14kN  15kN  15kN  16kN  16kN  17kN  17kN  19kN  19kN  19kN  19kN  20kN  20kN  21kN  21kN  22kN  22kN  23kN  23kN  24kN  24kN  27kN  27kN  31kN  31kN  34kN  34kN  37kN  37kN  39kN  39kN  43kN  43kN  47kN  47kN  49kN  49kN  53kN  53kN  58kN  58kN  64kN  64kN  81kN  98kN 114kN 128kN  
100.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   3kN   3kN   3kN   3kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  11kN  11kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  18kN  18kN  18kN  18kN  19kN  19kN  20kN  20kN  21kN  21kN  22kN  22kN  23kN  23kN  26kN  26kN  29kN  29kN  42kN  42kN  38kN  38kN  40kN  40kN  42kN  42kN  45kN  45kN  47kN  47kN  48kN  48kN  51kN  51kN  57kN  57kN  72kN  87kN 102kN 118kN  
105.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   3kN   3kN   7kN   7kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  13kN  13kN  14kN  14kN  15kN  15kN  17kN  17kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  21kN  21kN  22kN  22kN  25kN  25kN  28kN  28kN  38kN  38kN  36kN  36kN  40kN  40kN  41kN  41kN  42kN  42kN  43kN  43kN  45kN  45kN  47kN  47kN  50kN  50kN  60kN  74kN  89kN 107kN
110.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   3kN   3kN   6kN   6kN   7kN   7kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  16kN  16kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  21kN  21kN  24kN  24kN  26kN  26kN  30kN  30kN  32kN  32kN  35kN  35kN  36kN  36kN  37kN  37kN  38kN  38kN  39kN  39kN  40kN  40kN  46kN  46kN  59kN  72kN  86kN  99kN
115.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   3kN   3kN   5kN   5kN   6kN   6kN   8kN   8kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  16kN  16kN  16kN  16kN  18kN  18kN  18kN  18kN  19kN  19kN  20kN  20kN  22kN  22kN  24kN  24kN  30kN  30kN  32kN  32kN  33kN  33kN  34kN  34kN  35kN  35kN  36kN  36kN  37kN  37kN  38kN  38kN  40kN  40kN  53kN  66kN  79kN  91kN
120.0km/h 0.0kN   1kN   1kN   1kN   1kN   2kN   2kN   2kN   2kN   2kN   2kN   4kN   4kN   5kN   5kN   7kN   7kN   9kN   9kN  10kN  10kN  11kN  11kN  12kN  12kN  13kN  13kN  14kN  14kN  15kN  15kN  15kN  15kN  16kN  16kN  17kN  17kN  18kN  18kN  19kN  19kN  20kN  20kN  21kN  21kN  22kN  22kN  23kN  23kN  24kN  24kN  25kN  25kN  26kN  26kN  27kN  27kN  28kN  28kN  31kN  31kN  33kN  33kN  37kN  37kN  50kN  61kN  74kN  85kN
 ) ) 
 
 
Comment ( "Brzdovy system DAKO, brzdice DAKO BS2, DAKO BP, kompresor 3DSK-100" )
Comment ( "Brzdeni I.zpusob, rezim brzdeni P" )
BrakesEngineBrakeType ( "Air_single_pipe" )
BrakesTrainBrakeType ( "Air_single_pipe" )
BrakesEngineControllers ( "Independent, Train" )
DoesBrakeCutPower ( 1 )   

ORTSMainResChargingRate ( 0.06bar/s )
ORTSBrakePipeChargingRate ( 20.7bar/s ) 
AirBrakesMainMinResAirPressure ( 7.2bar )
AirBrakesMainMaxAirPressure ( 10bar )
AirBrakesMainResVolume ( 1000l )
AirBrakesAirCompressorWattage ( 35000W )
AirBrakesCompressorRestartPressure ( 8.5bar )
AirBrakesIsCompressorElectricOrMechanical ( 0 )
ORTSTrainPipeLeakRate ( 0.0042bar/s ) 

ORTSEngineBrakeReleaseRate ( 1.0bar/s )
ORTSEngineBrakeApplicationRate ( 1.3bar/s )
EngineBrakesControllerMinPressureReduction ( 0.3bar )
EngineBrakesControllerFullServicePressureDrop ( 1.0bar )
EngineBrakesControllerMaxApplicationRate ( 1.33bar/s )
EngineBrakesControllerMaxReleaseRate ( 1.0bar/s )
EngineBrakesControllerMaxSystemPressure ( 5bar )  

TrainBrakesControllerMinPressureReduction ( 0.3bar )
TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
TrainBrakesControllerMaxReleaseRate ( 0.5bar/s )
TrainBrakesControllerMaxApplicationRate ( 0.5bar/s )
TrainBrakesControllerMaxQuickReleaseRate ( 2.0bar/s )
TrainBrakesControllerEmergencyApplicationRate ( 1.86bar/s )
TrainBrakesControllerMaxSystemPressure ( 5bar )

	DynamicBrakesResistorCurrentLimit    ( 3581 )
	DynamicBrakesDelayTimeBeforeEngaging   ( 3 )
	DynamicBrakesNumberOfControllerNotches   ( 36 )
	DynamicBrakesMaxAirBrakePressure    ( 20 )
	DynamicBrakeHasAutoBailOff      ( 1 )
	DynamicBrakesMaximumForce      ( 724kN )
	DynamicBrakesLowerSpeedCurveExponent   ( 1 )
	DynamicBrakesMinUsableSpeed      ( 6.21 )
	DynamicBrakesFadingSpeed      ( 80.78 )
	DynamicBrakesMaximumEffectiveSpeed    ( 80.78 )
	DynamicBrakesMaximumSpeedForFadeOut    ( 80.78 )
	DynamicBrakesEffectAtMaximumFadeOut    ( 0 )
	DynamicBrakesCutInSpeed       ( 6.21 )
	DynamicBrakesCutOutSpeed       ( 6.21 )
	DynamicBrakesHigherSpeedCurveExponent   ( 1 )	

ORTSBrakePipeTimeFactor ( 0.003 )
ORTSBrakeServiceTimeFactor ( 1.009 )
ORTSBrakeEmergencyTimeFactor ( 0.1 ) 

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Dynamic" )

comment ( Monitors )


 VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 27 )
  MonitoringDeviceAlarmTimeLimit ( 17 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
  MonitoringDeviceResetOnDirectionNeutral ( 1 )
 )
 OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 72.6 )
  MonitoringDeviceResetLevel ( 0 )
  Comment ( MonitoringDeviceTriggerOnHighCurrent ( 1250 ) )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 0 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 0 )
  MonitoringDeviceDoesSuppressionReset ( 0 )
  MonitoringDeviceTriggerOnOverspeed ( 68.5 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 0 )
 )
		
	 
Comment	( Controllers )

        EngineControllers (
		Throttle ( 0 1 0.001 0
			NumNotches ( 69
			    Notch ( 0.0   0 Dummy )
			    
			    Notch ( 0.01  0 Dummy )
			    Notch ( 0.011 0 Dummy )
			    
			    Notch ( 0.02  0 Dummy )
			    Notch ( 0.021 0 Dummy )
			    
			    Notch ( 0.025 0 Dummy )
			    Notch ( 0.026 0 Dummy )
			    
			    Notch ( 0.03  0 Dummy )
			    Notch ( 0.031 0 Dummy )
			    
			    Notch ( 0.04  0 Dummy )
			    Notch ( 0.041 0 Dummy )
			    
			    Notch ( 0.05  0 Dummy )
			    Notch ( 0.051 0 Dummy )
			    
			    Notch ( 0.08  0 Dummy )
			    Notch ( 0.081 0 Dummy )
			    
			    Notch ( 0.1   0 Dummy )
			    Notch ( 0.101 0 Dummy )
			    
			    Notch ( 0.12  0 Dummy )
			    Notch ( 0.121 0 Dummy )
			    
			    Notch ( 0.14  0 Dummy )
			    Notch ( 0.141 0 Dummy )
			    
			    Notch ( 0.16  0 Dummy )
			    Notch ( 0.161 0 Dummy )
			    
			    Notch ( 0.19  0 Dummy )
			    Notch ( 0.191 0 Dummy )
			    
			    Notch ( 0.21  0 Dummy )
			    Notch ( 0.211 0 Dummy )
			    
			    Notch ( 0.24  0 Dummy )
			    Notch ( 0.241 0 Dummy )
			    
			    Notch ( 0.26  0 Dummy )
			    Notch ( 0.261 0 Dummy )
			    
			    Notch ( 0.29  0 Dummy )
			    Notch ( 0.291 0 Dummy )
			    
			    Notch ( 0.32  0 Dummy )
			    Notch ( 0.321 0 Dummy )
			    
			    Notch ( 0.35  0 Dummy )
			    Notch ( 0.351 0 Dummy )
			    
			    Notch ( 0.37  0 Dummy )
			    Notch ( 0.371 0 Dummy )
			    
			    Notch ( 0.40  0 Dummy )
			    Notch ( 0.401 0 Dummy )
			    
			    Notch ( 0.43  0 Dummy )
			    Notch ( 0.431 0 Dummy )
			    
			    Notch ( 0.46  0 Dummy )
			    Notch ( 0.461 0 Dummy )
			    
			    Notch ( 0.48  0 Dummy )
			    Notch ( 0.481 0 Dummy )
			    
			    Notch ( 0.51  0 Dummy )
			    Notch ( 0.511 0 Dummy )
			    
			    Notch ( 0.54  0 Dummy )
			    Notch ( 0.541 0 Dummy )
			    
			    Notch ( 0.58  0 Dummy )
			    Notch ( 0.581 0 Dummy )
			    
			    Notch ( 0.61  0 Dummy )
			    Notch ( 0.611 0 Dummy )
			    
			    Notch ( 0.64  0 Dummy )
			    Notch ( 0.641 0 Dummy )
			    
			    Notch ( 0.67  0 Dummy )
			    Notch ( 0.671 0 Dummy )
			    
			    Notch ( 0.70  0 Dummy )
			    Notch ( 0.701 0 Dummy )
 
			    Notch ( 0.73  0 Dummy )
			    Notch ( 0.731 0 Dummy )
			    
			    Notch ( 0.75  0 Dummy )
			    Notch ( 0.751 0 Dummy )
			    
			    Notch ( 0.81  0 Dummy )
			    Notch ( 0.86  0 Dummy )
			    Notch ( 0.92  0 Dummy )
			    Notch ( 1     0 Dummy )
		)
	)           

		
	comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 0.8 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
        comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 7
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
    
    
                Brake_Dynamic  ( 0 1 0.001 0
			NumNotches ( 48
			    Notch ( 0.0   0 Dummy )
			    Notch ( 0.001   0 Dummy )
			    
			    Notch ( 0.01  0 Dummy )
			    Notch ( 0.011 0 Dummy )
			    
			    Notch ( 0.02  0 Dummy )
			    Notch ( 0.021 0 Dummy )
			    
			    Notch ( 0.025 0 Dummy )
			    Notch ( 0.026 0 Dummy )
			    
			    Notch ( 0.03   0 Dummy )
			    Notch ( 0.031 0 Dummy )
			    
			    Notch ( 0.04  0 Dummy )
			    Notch ( 0.041 0 Dummy )
			    
			    Notch ( 0.05   0 Dummy )
			    Notch ( 0.051 0 Dummy )
			    
			    Notch ( 0.08  0 Dummy )
			    Notch ( 0.081 0 Dummy )
			    
			    Notch ( 0.1   0 Dummy )
			    Notch ( 0.101 0 Dummy )
			    
			    Notch ( 0.12  0 Dummy )
			    Notch ( 0.121 0 Dummy )
			    
			    Notch ( 0.14  0 Dummy )
			    Notch ( 0.141 0 Dummy )
			    
			    Notch ( 0.16   0 Dummy )
			    Notch ( 0.161 0 Dummy )
			    
			    Notch ( 0.19  0 Dummy )
			    Notch ( 0.191 0 Dummy )
			    
			    Notch ( 0.21  0 Dummy )
			    Notch ( 0.211 0 Dummy )
			    
			    Notch ( 0.24  0 Dummy )
			    Notch ( 0.241 0 Dummy )
			    
			    Notch ( 0.26  0 Dummy )
			    Notch ( 0.261 0 Dummy )
			    
			    Notch ( 0.29   0 Dummy )
			    Notch ( 0.291 0 Dummy )
			    
			    Notch ( 0.32  0 Dummy )
			    Notch ( 0.321 0 Dummy )
			    
			    Notch ( 0.35  0 Dummy )
			    Notch ( 0.351 0 Dummy )
			    
			    Notch ( 0.37  0 Dummy )
			    Notch ( 0.371 0 Dummy )
			    
			    Notch ( 0.40  0 Dummy )
			    Notch ( 0.401 0 Dummy )
			    
			    Notch ( 0.43   0 Dummy )
			    Notch ( 0.431 0 Dummy )
			    
			    Notch ( 0.46  0 Dummy )
			    Notch ( 0.461 0 Dummy )
			    
			    Notch ( 0.48  0 Dummy )
			    Notch ( 0.481 0 Dummy )
			    
	       		)
  		)
	       Combined_Control( 0 1 1 1 throttle dynamic )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	
  	
comment	( CabSound and Views )

	Sound ( "..\\..\\common.snd\\sndelok\\240cab.sms" )
	
	CabView ( "240zscs.cvf" )

	HeadOut (1.7 3.2 5.7 )
	
	
Comment	( Operations )


	 Name ( "ZSCS 240 082-8 " )
	 Description (
	  "Rada 240 ZSCS je univerzální elektrická skrínová lokomotiva, pouzívaná v nákladní doprave.\n\n"+
	  "Typ Bo'-Bo', napeti 25 kV 50Hz.\n\n"+
	  "Délka pres nárazniky: 16,44 m\n\n"+
	  "Prumer hnacích kol: 1250 mm\n\n"+
	  "Hmotnost ve sluzbe: 84.5 t\n\n"+
	  "Trvaly vykon trakcních motoru: 3080 kW\n\n"+
	  "Max. rychlost 110 km/h\n\n"+
	  "Ovladani a proudy v MSTS:\n\n"+
	  "Maximalni proud (nadproudova ochrana): 1250A\n\n"+
	  "Trvaly proud: 1100A\n\n"+
	  "Hodinovy proud: 1140A\n\n"+
	  "15 minutovy proud: 1300A\n\n"+
	  "5 minutovy proud: 1500A\n\n"+
	  "Proud na mezi adheze (skluz): 1548A\n\n"+
	  "Proud na mezi adheze s piskovanim (skluz): 1961A\n\n"+
	  "Kontroler: 32 stupnu (1%-75%) + 4 shuntovaci (81%-100%)\n\n"+
	  "EDB: 23 stupnu (1%-48%)\n\n"+
	  "Maximalni vykon EDB: 2000kW\n\n"+
	  "Maximalni proud kotvy EDB pri rychlosti  57km/h: 760A\n\n"+	  
	  "Maximalni proud kotvy EDB pri rychlosti  80km/h: 544A\n\n"+
	  "Maximalni proud kotvy EDB pri rychlosti 100km/h: 438A\n\n"+
	  "Maximalni proud kotvy EDB pri rychlosti 120km/h: 333A\n\n"+
	  "Maximalni proud buzeni EDB: 1250A\n\n"+
	  "Maximalni proud buzeni EDB na meraku, ktery nesmite prekrocit!: 760A\n\n"
	 )

	 EngineOperatingProcedures (
	  "Jak se rozjet\n"+
	  "1. Uz máte zvednutý pantograf. (Pokud z nejakého duvodu zvednutý není, stisknete klávesu P pro jeho zvednutí.)\n"+
	  "2. Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
	  "3. Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
	  "(4. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
	  "5. Stisknete D pro zvýsení pozadovaného výkonu.\n"+
	  "6. Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n\n"+
	  "Jak zpomalit\n"+
	  "1. Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
	  "2. Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
	  "Jak pouzít vlakovou brzdu\n"+
	  "1. Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
	  "2. Po dosazení pozadovaného brzd. tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
	  "Jak odbrzdit vlakovou brzdu\n"+
	  "1. Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
	  "2. Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
	  "3. Stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n"+
	  "Jak pouzít lokomotvní brzdu\n"+
	  "1. Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak odbrzdit lokomotivní brzdu\n"+
	  "1. Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0-100%).\n\n"+
	  "Jak pouzít zachrannou brzdu\n"+
	  "1. Stisknete a drzte A pro snízení výkonu az na 0.\n"+
	  "2. Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
	  "Jak zrusit záchrannou brzdu\n"+
	  "1. Pockejte na úplné zastavení vlaku.\n"+
	  "2. Stisknete Z pro odblokování ovládání lokomotivy.\n"+
	  "3. Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
	  "4. Pomalu zvysujte výkon stiskem D .\n\n"+
	  "Jak zmenit smer\n"+
	  "1. Zastavte vlak.\n"+
	  "2. Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
	  "3. Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
	  "4. Pomalu zvysujte vykon stiskem D .\n\n"+
	  "Jak pripojit vagony/lokomotivy\n"+
	  "1. K vagonu musíte prijet pomalu, optimální rychlost je okolo 1 km/h.\n"+
	  "Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
	  "2. Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
	  "3. Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
	  "4. Zavrete okno sestavení vlaku stiskem F9.\n"+
	  "5. Pockejte az odbrzdíte pripojené vozy.\n\n"+
	  "Odpojení vozu nebo lokomotivy\n"+
	  "POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"+
	  "1. Otevrete okno sestavy vlaku F9.\n"+
	  "2. Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
	  "3. Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
	  "4. Pomalu se rozjedte smerem od odpojene casti vlaku.\n"+
	  "(Pozn.: V nekterých prípadech pri rychlejsím odjezdu dojde k opetovnému spojení spráhel. Pokud se toto stane tak soupravu opet rozpojte a velmi pomalu odjízdejte az do vzdálenosti jednoho prazce. Pak jiz muzete zacít zrychlovat.)\n"+
	  "5. Zavrete okno sestavení vlaku stiskem F9.\n\n"
	 ) 
)