SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( zsr_850018
		comment( upravil Ondra Janis na zaklade poznatku o ladeni eng 
  souboru od Ppoolllla, Jacka, O.Frinty & ZSR  - verze 1.0 )
	Type ( Engine )
	WagonShape ( "zsr_850018.s" )
	Size ( 3.0m 4.2m 24.49m )
	Mass ( 55.0t )
	comment(53t + cca. 1/2 obsazeni, plne obsazeny vuz 56,5t)
	WheelRadius ( 0.45m )
	InertiaTensor ( Box (3.0m 4.2m 24.49m) )
	Freightanim ( "zsr_850018fg.s" 1 1 )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	
	Adheasion ( 0.05 0.29 0.83 0 )
comment (melo by odpovidat adhezni sile pro 850 ~65kN)
	DerailRailHeight ( 8cm )
	DerailRailForce ( 2.5*55t )
	DerailBufferForce ( 1200kN )
comment( pocet naprav )
	NumWheels (	4 )
comment( sily urcujici jizdni odpory )
	Friction (
		1720N/m/s		0		0.625mph		0.99N/m/s		2.5
		5.1N/rad/s		1		-1rad/s		0		1
	)

	BrakeEquipmentType( "Handbrake, Graduated_release_Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 55kN )
	MaxHandbrakeForce( 8kN )
	NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.3 )
	MaxApplicationRate( 4 )
	MaxAuxilaryChargingRate( 3 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
	EmergencyResVolumeMultiplier ( 8 )
	EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate ( 1 )
	EmergencyBrakeResMaxPressure( 73 )
	
	IntakePoint ( 0 1.0 FuelDiesel )

	PassengerCapacity ( 80.0 )
	comment(48 mist k sezeni + odhad mist k stani)

	Lights ( 23
		Light (
			comment ( Svetelny kuzel dalkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffEED15D )
					Position ( 0.0 3.71 11.80 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 120 )
				)
			)
		)
		Light (
			comment ( Svetelny kuzel tlumeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.0 1.484 11.880 )
					Angle ( 30 )
					Transition ( 1 )
					Radius ( 80 )
				)
			)
		)

		comment ( Definice svetel pro predni stanoviste )

		Light (
			comment ( reflektor dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffEED15D )
					Position ( 0.0 3.71 11.80 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
                Light (
			comment ( reflektor tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFE085 )
					Position ( 0.0 3.71 11.80 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
		Light (
			comment ( predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.851 1.484 11.880 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.851 1.484 11.880 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		
		comment ( Definice svetel pro zadni stanoviste )

		Light (
			comment ( reflektor dalkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( ffEED15D )
					Position ( 0.0 3.71 -11.80 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
                Light (
			comment ( reflektor tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFE085 )
					Position ( 0.0 3.71 11.80 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.851 1.484 11.880 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.851 1.484 11.880 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

                Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.851 1.484 11.880 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( zadni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
                
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Prave predni pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.851 1.484 11.880 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		comment ( Definice svetel pro loko ovladanou PC )

		Light (
			comment ( PC predni prave )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.851 1.484 11.880 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( PC predni leve )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.851 1.484 11.880 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( PC reflektor predni 1 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.0 3.71 11.80 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
		Light (
			comment ( PC zadni leve koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( PC zadni prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.851 1.484 -11.880 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
				)
			)
		)
	)
      	Sound ( "../../common.snd/sndMlok/850eng.sms" )
	)

Engine ( zsr_850018
	Effects (
		DieselSpecialEffects (
			Exhaust1
				(
					0.0 4.2 9.691
					0 1 0
					0.1
				)
		)
	)
		 DieselSmokeEffectInitialMagnitude( 0.2 )
		 DieselSmokeEffectMaxMagnitude( 1 )
		 DieselSmokeEffectInitialSmokeRate( 0.2 )
		 DieselSmokeEffectMaxSmokeRate( 1 )

	Wagon ( zsr_850018 )
	Type ( Diesel )
	MaxPower ( 377kW ) 
      comment (vykon na obvodu kol - vypocteno z trakcni char.) 
	MaxForce ( 77kN )
	    comment (nejde o skutecnou max. taznou silu, ale kompromis pro taznou silu na jednotlive stupne -
      pri tazne sile ~68kN dojde k dosazeni meze adheze a prokluzu)
	RunUpTimeToMaxForce ( 10.0 )
	MaxContinuousForce ( 77kN )
	MaxVelocity ( 110km/h )
	MaxCurrent ( 600A ) 
	WheelRadius ( 0.45m )
	Sanding ( 19km/h )
	NumWheels ( 2 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )
	DieselEngineSpeedOfMaxTractiveEffort( 18 km/h )
	
	AirBrakesAirCompressorPowerRating( 0.3 )
	AirBrakesMainMinResAirPressure( 56 )
	AirBrakesMainMaxAirPressure( 116 )
	AirBrakesMainResVolume( 20 )
	AirBrakesAirCompressorWattage( 10kW )
	AirBrakesCompressorRestartPressure( 108.75 )

	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.4 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1 )
	TrainBrakesControllerMaxReleaseRate ( 0.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 3 )
	TrainBrakesControllerMinSystemPressure ( 3 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )

		
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Independent, Train" )

	EngineBrakesControllerDirectControlExponent( 1 )

 	CabView ( "..//..//common.cab//cab850-018//850-018_M.cvf" )
	HeadOut ( 1.75 2.6 10.5 )

 	MaxDieselLevel ( 1600l )
  DieselUsedPerHourAtMaxPower ( 168l )
	DieselUsedPerHourAtIdle ( 18l )

	DieselSmokeEffectInitialMagnitude( 0.7 )
	DieselSmokeEffectMaxMagnitude( 1.2 )

	DieselSmokeEffectInitialSmokeRate( 0.8 )
	DieselSmokeEffectMaxSmokeRate( 2.2 )

	DieselEngineIdleRPM( 700 )
	DieselEngineMaxRPM( 1470 )

  DieselEngineMaxRPMChangeRate( 35 )

	DoesHornTriggerBell( 0 )

	MaxSandingTime( 2000 )
	comment( 320kg )

	EmergencyStopMonitor(
    MonitoringDeviceMonitorTimeLimit( 0 )
    MonitoringDeviceAlarmTimeLimit( 0 )
    MonitoringDevicePenaltyTimeLimit( 0 )
    MonitoringDeviceCriticalLevel( 0 )
    MonitoringDeviceResetLevel( 0 )
    MonitoringDeviceAppliesFullBrake( 0 )
    MonitoringDeviceAppliesEmergencyBrake( 1 )
    MonitoringDeviceAppliesCutsPower( 1 )
    MonitoringDeviceAppliesShutsDownEngine( 1 )
    )

		
	OverSpeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		)
	
		
	EngineVariables( 4000 )
			
        EngineControllers (
            Throttle ( 0 1 0.12 0 
                NumNotches ( 8
                    Notch ( 0        0 Dummy )
                    Notch ( 0.15    0 Dummy )
                    Notch ( 0.28    0 Dummy )
                    Notch ( 0.42    0 Dummy )
                    Notch ( 0.55    0 Dummy )
                    Notch ( 0.68    0 Dummy )
                    Notch ( 0.849  0 Dummy )
                    Notch ( 0.850  0 Dummy )
                )
            )
            Brake_Engine ( 0 0.76 0.125 0
                NumNotches( 1
                    Notch(0    1 Dummy )
                )
            )                 
            comment(***Prubezna brzda typ DAKO-BS2***)            
           	Brake_Train ( 0 1 0.020 0.87
                NumNotches ( 7
                    Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
                    Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
                    Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 1.00 0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
            NumNotches( 1
                    Notch(0    1 Dummy)
                )
            )
            DirControl ( -1 0 1 1 )
            AWS ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
	     )
        
    	Name ("ZSR 850 018-3")
    	Description (
	 "Motorovy vuz 850 ZSSK\n\n"+
	 "Univerzalni motorovy vuz pro \n"+
	 "osobni, spesne vlaky i rychliky "+
	 "na neelektrizovanych tratich. "+
	 "V soucasne dobe je u ZSSK posledni provozni exemplar.\n\n"+  
	 "Prenos vykonu: hydraulicky, pres MMM prevodovku\n\n"+
	 "Motor: CKD K 12 V 170 DR \n\n"+
	 "Vykon: 515 kW pri 1400 min-1 \n\n"+
	 "Max. rychlost: 110 km/h\n\n"+
	 "Delka pres narazniky: 24790 mm\n\n"+
	 "Hmotnost: 53 - 57 t\n\n"+
	 "Napravy: 4, usporadani B'2'\n\n"+
	 "Vyroba: Vagonka Studenka, 1967"
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestaveni reverzniho kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdeni vlakove brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy.)\n"+
		"4.	Stisknete D pro zvyseni pozadovaneho vykonu.\n"+
		"5.	Pomalu zvysujte vykon stiskem D, dokud vlak nedosahne pozadovane rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jednim stiskem ' presunte vlakovou brzdu do polohy ZaVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snizeni pozadovaneho vykonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutne tak pouzijte brzdy pro postupne rychlejsi snizovani rychlosti.\n\n"+
		"Jak pouzit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosahnete pozadovaneho brzdneho tlaku.\n"+
		"2.	Po dosazeni pozadovaneho brzdneho tlaku stiskem ; presunte rukojet brzdy do polhy ZaVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENi.\n"+
		"2.	Pockejte, az klesne tlak v brzdovych valcich na 0.\n"+
		"3.	Po odbrzdeni a uvedeni vlaku do pohybu stisknete ' pro presunuti rukojeti brzdy do polohy ZaVER.\n\n"+
 		"Jak pouzit lokomotvni brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdeni lokomotivni brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivni brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdeni lokomotivni brzdy (0%).\n\n"+
		"Jak pouzit zachrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snizeni vykonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci zachrane brzdy.\n\n"+
		"Jak zrusit zachrannou brzdu\n"+
		"1.	Pockejte na uplne zastaveni vlaku.\n"+
		"2.	Stisknete Z pro odblokovani ovladani lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdeni brzdnych systemu.\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitym stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (pripadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Vystup a nastup cestujicich\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahajeni vystupu a nastupu cestujicich.\n"+
		"3.	Pockejte na signal k odjezdu.\n"+
		"TIP: Pro zobrazeni casu prijezdu a odjezdu u teto a nasledujici stanice pouzijte klavesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimalni rychlost 1 km/h).\n"+
		"Tip: Pro zobrazeni pohledu na sprahlo stisknete klavesu 6.\n"+
		"2.	Stisknete F9 pro otevreni okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervena, je zatazena rucni brzda. Dvojtukem mysi na voze uvolnite/zatahne rucni brzdu.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdite pripojene vozy.\n\n"+
		"Odpojeni vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provadet jen tehdy, pokud VLAK STOJi!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se ma odpojit, pokud chcete, aby mel vuz zatazenou rucni brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestaveni vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftoveho stojanu stredem nadrze.\n"+
		"2.	Stisknete klavesu T a drzte ji po dobu doplnovani nafty stisknutou.\n"+
		"TIP: Pro zobrazeni prubehu plneni nadrze stisknete F9 a klepnete mysi na ikonu lokomotivy.\n\n"+
	)
	Sound ( "../../common.snd/sndMlok/850cabP.sms" )
)
