SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( CD_742083rv
	Type ( Engine )
	WagonShape ( CD_742083rv.s )
	
comment	( Overall physics )


	Size ( 3.00m 4.42m 13.30m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 64.0t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.00m 4.42m 13.30m ) )


comment	( Coupling )

Coupling (
	Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 1.5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 1.5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e7N/m 0 )
			Damping ( 1e6N/m/s 0 )
			r0 ( 60cm 30cm )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)
	


comment	( Adhesion and Friction )

	Adheasion ( 0.19 0.805 1.11 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*73t )
	DerailBufferForce ( 800kN )
	NumWheels (	4 )
	Friction (
		2500N/m/s		0		1mph		11N/m/s		1.9
		5.1N/rad/s		1		-1rad/s		0		1
	)



comment	( Wagon Brakes )

 	Comment ( P=42kN, G=30kN )
 	
	MaxBrakeForce( 42kN )
	MaxHandbrakeForce( 10kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 2 )
	MaxApplicationRate( 3 )
	MaxAuxilaryChargingRate( 3 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
        EmergencyResVolumeMultiplier ( 11 )
        EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 ) 
	
comment	( EngSound, Freight, Inside, IntakePoint )

	Sound ( "../../common.snd/snd742.159/742.159ng.sms"  )
    	
	IntakePoint ( 0 2 FuelDiesel )


      	Inside (
		PassengerCabinFile ( CD_742083rv.s )
		PassengerCabinHeadPos ( -1.7 3.0 3.37 )
		RotationLimit ( 0 190 0 )
		StartDirection ( 0 0 0 )
	)

comment	( Lights )


 Comment ( svetla neznamsebe - 1 dalkove svetlo velke, obdobi od 1997 )
	Lights ( 31
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0 3.8 6.0 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 400 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0 3.8 6.0 )
					Angle ( 30 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)

		comment ( Definice svetel pro prední stanoviste )

		Light (
			comment ( reflektor dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.0 3.816 6.03 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.0 3.816 6.03 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( Prední levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( -0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( 0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( -0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( 0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( -0.7 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( 0.7 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.7 1.83 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.7 1.83 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.0 3.816 -6.03 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.0 3.816 -6.03 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( Prední levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( -0.7 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( 0.7 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( -0.7 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( 0.7 2.088 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( -0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFFFDF )
					Position ( 0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.7 1.83 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.7 1.83 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.22 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Levé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 )
					Position ( -0.7 2.088 6.05 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 )
					Position ( 0.7 2.088 6.05 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 )
					Position ( -0.7 2.088 -6.05 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Pravé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFE085 )
					Position ( 0.7 2.088 -6.05 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
					)
			)
		)

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFE085 )
					Position ( 0.7 2.088 6.05 )
					Azimuth ( 0 -5 5 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 70FFE085 )
					Position ( -0.7 2.088 6.05 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( PC reflektor prední )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.0 3.797 7.835 )
					Azimuth ( 0 0 5 )
					Transition ( 1 )
					Radius ( 0.9 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.7 1.83 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.7 1.83 -6.05 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
     )
    )
   )
  )
)


Engine ( CD_742083rv

comment	( Description )

	Wagon ( CD_742083rv )

	
comment	( Basic physical engine data )

	Type ( Diesel )
	MaxPower ( 645kW )
	MaxForce ( 215kN )	
	MaxContinuousForce ( 215kN )
	MaxCurrent ( 2250A ) 
	MaxVelocity ( 54.4mph )
	DieselEngineSpeedOfMaxTractiveEffort( 6.92mph )  
	WheelRadius ( 0.5m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 1e9mph )
	NumWheels ( 4 )
	
	
comment	( CabSound and Views )

 	Sound ( "../../common.snd/snd742.159/742.159cab.sms"  )
 	
 	CabView ( "../../common.cab/cab740_742/742rv.cvf" )

	HeadOut ( 1.7 3.0 3.37 )
	
comment	( Diesel Engine )

	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )

	DieselEngineIdleRPM( 400 )
	DieselEngineStallRPM( 400 )	
	DieselEngineMaxRPM( 1250 )
	DieselEngineMaxRPMChangeRate( 55 )
	RunUpTimeToMaxForce ( 50 )

comment	( Transmission and GearBox )

	DieselEngineType ( electric )



comment	( Fuel and Usage )

	MaxDieselLevel ( 4000l )
	DieselUsedPerHourAtMaxPower ( 230l )
	DieselUsedPerHourAtIdle ( 12.3l )


comment	( Smoke and Steam )

	 Effects
	  (
	  DieselSpecialEffects
	   (
	    comment
	    (
	     the format of these little blocks is as follow:

	     offset.x offset.y offset.z
	     normal.x normal.y normal.z
	     width in metres

	     defining the offset from the shape pivot point
	     where steam / smoke should appear, the direction
	     it should go and the width of the nozzle
	    )

	    Exhaust1
	    (
	     0.0 4.6 1.25
	     0 1 0
	     0.1
	    )
	   )
         )


	 DieselSmokeEffectInitialMagnitude( 0.3 )
	 DieselSmokeEffectMaxMagnitude( 3.2 )
	 DieselSmokeEffectInitialSmokeRate( 0.25 )
	 DieselSmokeEffectMaxSmokeRate( 3.56 )


comment	( Brakes )


	AirBrakesAirCompressorPowerRating ( 1.55 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 145 )	
	AirBrakesMainResVolume ( 35.315 )
	AirBrakesAirCompressorWattage ( 20474 )
	AirBrakesCompressorRestartPressure ( 120 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 2 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 2 )
	TrainBrakesControllerMaxApplicationRate ( 1.8 )
	TrainBrakesControllerMaxReleaseRate ( 2.0 )
	TrainBrakesControllerMaxQuickReleaseRate ( 5.0 )
	TrainBrakesControllerEmergencyApplicationRate ( 10 )
	TrainBrakesControllerMinSystemPressure ( 3 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

comment ( Monitors )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 20 )
  MonitoringDeviceAlarmTimeLimit ( 10 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
 )
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 58.9 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 0 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 59.0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)

EngineVariables( 1000 )

comment	( Controllers )

        EngineControllers (
             Throttle ( 0 1 0.125 0
			NumNotches ( 9
				Notch ( 0    0 Dummy )
				Notch ( 0.03 0 Dummy )
				Notch ( 0.05 0 Dummy )
				Notch ( 0.18 0 Dummy )
				Notch ( 0.32 0 Dummy )
				Notch ( 0.46 0 Dummy )
				Notch ( 0.62 0 Dummy )
				Notch ( 0.83 0 Dummy )
				Notch ( 1    0 Dummy )
			)
		)         
		comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 0.76 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
            comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 7
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)

            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	
Comment	( Operations )


    	Name ( "CD 742.083-9 obracena" )
    	Description (
	 "Rada 742 CD je univerzalni dieselelektricka kapotova lokomotiva"+
	 "pro pouziti od posunovaciho provozu pres tazeni osobnich"+
	 "az do tazeni stredne tezkych nakladnich vlaku v dvojclennem rizeni.\n\n"+
	 "Usporadani dvojkoli: B0'B0'\n\n"+
	 "Prenos vykonu: elektricky\n\n"+
	 "Zdroj vykonu: naftovy motor CKD K 6 S 230 DR\n\n"+
	 "Vykon spalovaciho motoru: 883kW\n\n"+
	 "Max. provozni rychlost:  90km/h\n\n"+
	 "Trvala tazna sila na haku: 121kN pri 1200A\n\n"+
	 "Max. vyska: 4450mm\n\n"+
	 "Delka pres nar.: 13600mm\n\n"+
	 "Max. sirka: 3060mm\n\n"+
	 "Hmotnost plne vyzbroj. lokomotivy: 64t"  
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
		"4.	Stisknete D pro zvýsení pozadovaného výkonu.\n"+
		"5.	Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jedním stiskem ' presunte vlakovou brzdu do polohy ZÁVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
		"Jak pouzít vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
		"2.	Po dosazení pozadovaného brzdného tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
		"2.	Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
		"3.	Po odbrzdení a uvedení vlaku do pohybu stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n\n"+
 		"Jak pouzít lokomotvní brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivní brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0%).\n\n"+
		"Jak pouzít záchrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snízení výkonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
		"Jak zrusit záchrannou brzdu\n"+
		"1.	Pockejte na úplné zastavení vlaku.\n"+
		"2.	Stisknete Z pro odblokování ovládání lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
		"4.	Pomalu zvysujte výkon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Výstup a nástup cestujících\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahájení výstupu a nástupu cestujících.\n"+
		"3.	Pockejte na signál k odjezdu.\n"+
		"TIP: Pro zobrazení casu príjezdu a odjezdu u této a následující stanice pouzijte klávesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimální rychlost 1 km/h).\n"+
		"Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
		"2.	Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdíte pripojené vozy.\n\n"+
		"Odpojení vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftového stojanu stredem nádrze.\n"+
		"2.	Stisknete klávesu T a drzte ji po dobu doplnování nafty stisknutou.\n"+
		"TIP: Pro zobrazení prubehu plnení nádrze stisknete F9 a klepnete mysí na ikonu lokomotivy.\n\n"+
	)
)

