SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 81_54_0812_752_1_ko
Comment ( "Sekce vozidlo" )
Comment ( "Popis fyziky vozu pro OR" )
Comment ( "Josef Vogeltanz - 22.12.2019" )
Comment ( "Drobné úpravy pro vůz Taes Jakub H. - 4/2025" )

Comment ( "Obecne informace vozu" )
Type ( Freight )
WagonShape ( 81_54_0812_752_1.s )
Name ( "CDC Taes 0812 752-1 prazdny konce rv" )
Size ( 3.215m 4.38m 16.56m )
Mass ( 23.7t )
WheelRadius ( 0.46m )
NumWheels ( 4 )

ORTSFreightAnims (
MSTSFreightAnimEnabled ( 0 )
FreightAnimStatic ( 
SubType ( Default )
Shape ( bv_pr.s )
Offset ( 0.0, 0.0, 0.0 )
Flip ( 0 )
)
FreightAnimStatic ( 
SubType ( Default )
Shape ( konce_o.s )
Offset ( 0.0, 0.0, 0.0 )
Flip ( 0 )
)
)

Comment ( "Sprahla" )
Coupling (
Type ( Chain )
Spring ( Stiffness ( 4e5N/m 2.64e7N/m ) Break ( 8.5e5N 8.5e5N ) r0 ( 0cm 0.1cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Coupling (
Type ( Chain )
Spring ( Stiffness ( 4e5N/m 2.64e7N/m ) Break ( 8.5e5N 8.5e5N ) r0 ( 0cm 0.1cm ) )
CouplingHasRigidConnection ( 0 )
Velocity ( 0.01m/s ) )

Comment ( "Brzdy" )
Comment ( "Brzdovy system DAKO, zdrze, Bv.: 30t" )
Comment ( "Rezim brzdeni P" )
BrakeEquipmentType ( "Handbrake, Graduated_release_triple_valve, Auxilary_reservoir" )
BrakeSystemType ( "Air_single_pipe" )

MaxBrakeForce ( 92kN )
MaxHandbrakeForce ( 15kN )
NumberOfHandbrakeLeverSteps ( 10 )

TripleValveRatio ( 2.5 )
MaxReleaseRate ( 0.2bar/s )
MaxApplicationRate ( 0.45bar/s )
MaxAuxilaryChargingRate ( 1.621bar/s )
EmergencyResChargingRate ( 1.621bar/s )
BrakeCylinderPressureForMaxBrakeBrakeForce ( 3.8bar )
EmergencyResVolumeMultiplier ( 1.0 )
EmergencyResCapacity ( 75l )
BrakePipeVolume ( 14.5l )

ORTSBrakeShoeFriction ( 0 0.31 1 0.30 2 0.28 3 0.27 4 0.26 5 0.25 7 0.24 8 0.23 9 0.22 12 0.21 14 0.20 17 0.19 20 0.18 24 0.17 29 0.16 34 0.15 40 0.14 47 0.13 55 0.12 66 0.11 84 0.10 115 0.09 160 0.09 )

Comment ( "Jizdni odpory a treni" )
CentreOfGravity ( 0m 2.1m  0m )
ORTSTrackGauge ( 1m 435mm )
ORTSRigidWheelbase ( 1m 800mm )
ORTSUnbalancedSuperelevation ( 150mm )

ORTSBearingType ( Roller )
ORTSDavis_A ( 506.3 )
ORTSDavis_B ( 4.11 )
ORTSDavis_C ( 1.0541 )

Comment ( "Ostatni informace" )
Sound ( "..//..//common.snd//Vozy//CDvuzNakl4n-OR.sms" )
)