SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( LRL_620037
	Type ( Engine )
	WagonShape ( LRL_620037.s )
        ORTSFreightAnims
	(
        MSTSFreightAnimEnabled ( 0 )
				FreightAnimStatic
				(
				SubType( Default )
				Shape( "LRL_620037orfg.s" )
				Offset( 0.0, 0.0, 0.0 )
                                Visibility ( "Cab2D" )
				) 
                                FreightAnimStatic
				(
				SubType( Default )
				Shape( "LRL_620037fg.s" )
				Offset( 0.0, 0.0, 0.0 )
                                Visibility ( "Outside,Cab2D" )
				)
		)
Size ( 3.2m 4.597m 17.241m )
	CentreOfGravity ( 0m 2.3m 0m )
	Mass ( 115t )
	WheelRadius ( 0.5m )
 IntakePoint ( 0 2 FuelDiesel )
Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 6.7e6N/m 4.4e8N/m )
   Break ( 850kN 850kN )
   r0 ( 0cm 0cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 6.7e6N/m 4.4e8N/m )
   Break ( 850kN 850kN )
   r0 ( 0cm 0cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )
comment ( 12m2 )

ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        ORTSSlipWarningThreshold ( 100 )
        )
	NumWheels ( 6 )
	ORTSBearingType ( Roller )
        ORTSDavis_A ( 1506.97 )
        ORTSDavis_B ( 37.8408 )
        ORTSDavis_C ( 6.900120 )
comment (* odpor v oblouku *)
	ORTSTrackGauge ( 1435mm )
	comment (* rozvor podvozku *)
	ORTSRigidWheelbase ( 4000mm )
	ORTSUnbalancedSuperelevation ( 152.4mm )
comment	( =115t )

        BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType( "Air_single_pipe" )

        MaxBrakeForce( 123.75kN )

        TripleValveRatio( 2.33 )
	comment (** rezim P = 0.15625bar/s - odbrzdeni 22.4s **)
	comment (** rezim G = 0.07bar/s - odbrzdeni 50s **)
	MaxReleaseRate( 0.15625bar/s )
	comment (** rezim P = 0.660bar/s - zabrzdeni 5.3s **)
	comment (** rezim G = 0.159bar/s - zabrzdeni 22s **)
	MaxApplicationRate( 0.660bar/s )
	EmergencyResCapacity( 220l )
	EmergencyResVolumeMultiplier ( 1 )
	EmergencyBrakeResMaxPressure( 5bar )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 3.5bar )
  comment (** objem brzdoveho potrubi **)
BrakePipeVolume ( 0.52 )

        MaxHandbrakeForce( 9.96kN )
Comment (** Prubeh soucinitele treni dle rychlosti - litinove brzdove spalky - autor: Pajavlaky **)

ORTSBrakeShoeFriction (  	

		       0.0	0.3100
		       1.0	0.2800
		       2.0	0.2670
		       3.0	0.2572
		       4.0	0.2490
		       5.0	0.2419
		       6.0	0.2355
		       7.0	0.2296
		       8.0	0.2242
		       9.0	0.2192
		       10.0	0.2145
		       11.0	0.2100
		       12.0	0.2059
		       13.0	0.2019
		       14.0	0.1981
		       15.0	0.1945
		       16.0	0.1911
		       17.0	0.1878
		       18.0	0.1847
		       19.0	0.1817
		       20.0	0.1788
		       21.0	0.1760
		       22.0	0.1733
		       23.0	0.1708
		       24.0	0.1683
		       25.0	0.1660
		       26.0	0.1637
		       27.0	0.1615
		       28.0	0.1594
		       29.0	0.1574
		       31.0	0.1536
		       32.0	0.1518
		       33.0	0.1501
		       34.0	0.1484
		       35.0	0.1468
		       37.0	0.1439
		       38.0	0.1425
		       40.0	0.1399
		       41.0	0.1387
		       51.0	0.1277
		       57.0	0.1217
		       63.0	0.1163
		       68.0	0.1123
		       74.0	0.1080
		       80.0	0.1044
		       87.0	0.1009
		       94.0	0.0982
		       105.0	0.0949
		       120.0	0.0919
		       140.0	0.0897
		       160.0	0.0897

                      )

Sound ( "../../common.snd/snd770/770oreng.sms" )

Lights ( 28
		Light (
			comment ( Svetelny kuzel dialkovy )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFFFF )
					Position ( 0 4.098 7.4 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)
		Light (
			comment ( Svetelny kuzel tlmeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0 4.098 7.4 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 20 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( -0.116 4.03 7.4 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.116 4.03 7.4 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( reflektor lavy tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( -0.116 4.03 7.4 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0.116 4.03 7.4 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne lave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)		
		comment ( Definicia svetiel pre zadne stanoviste )
                Light (
			comment ( reflektor lavy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.116 4.03 -7.4 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkovy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( -0.116 4.03 -7.4 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
                Light (
			comment ( reflektor lavy tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0.116 4.03 -7.4 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( -0.116 4.03 -7.4 )
					Azimuth ( 180 180 180 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predne lave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( predne prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne lave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadne prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		
		comment ( Definicia svetiel pre Loose consist )

		Light	(
			comment( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Zadne lave pozicne)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		

		comment ( Definicia svetiel pre PC )

		Light (
			comment ( Predne prave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Predne lave pozicne )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                Light (
			comment ( reflektor lavy tlmeny )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( -0.116 4.03 7.4 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy tlmeny )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0.116 4.03 7.4 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Zadne lave pozicne )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Zadne prave pozicne )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
)
Engine ( LRL_620037

Type ( Diesel )
	MaxPower ( 885kW )
	MaxForce ( 310kN )	
	comment ( MaxContinuousForce ( 180kN ) )
	MaxCurrent ( 2340A ) 
	MaxVelocity ( 90km/h )
        ORTSSpeedOfMaxContinuousForce ( 16km/h )
	WheelRadius ( 0.5m )
	NumWheels ( 6 )
        ORTSDriveWheelWeight ( 115t )
 MaxDieselLevel ( 6000l )

ORTSDieselEngines ( 1
                Diesel (
                        IdleRPM ( 350 )
                        MaxRPM ( 750 )
                        StartingRPM ( 320 )
                        StartingConfirmRPM ( 351 )
                        ChangeUpRPMpS ( 38 )
                        ChangeDownRPMpS ( 26 )
                        RateOfChangeUpRPMpSS ( 100 )
                        RateOfChangeDownRPMpSS ( 100 )
                        MaximalPower ( 885kW )
                        IdleExhaust ( 0.12 )
                        MaxExhaust ( 2.15 )
                        ExhaustDynamics ( 1.6 )
                        ExhaustColor ( 206B787D )
                        ExhaustTransientColor ( 40212324 )
                        DieselPowerTab (
                                0  0
                                350  0
                                356  53100
                                380  70800
				420  132800
				460  239000
				510  389400
				560  513300
				660  717000
				750  885000
                        )
                        DieselConsumptionTab (
                                0  0
                                350  30.4
                                460  71.4
				510  103.6
				560  146.4
				660  214.3
				750  269.0
                        ) 
                        ThrottleRPMTab (
                                0  350
                                6  356
                                8  380
                                15  420
                                27  460
                                44  510
                                58  560
                                81  660
                                100  750
                        )
                        DieselTorqueTab (
                                0  0
                                350  818.57
                                356  1424.45
                                380  1779.32
				420  3018.48
				460  4960.81
				510  7291.71
				560  8753.6
				660  10373.33
				750  11269
                        )
                        MinOilPressure ( 36.20 )
                        MaxOilPressure ( 88 )
                        MaxTemperature ( 115 )
                        Cooling ( 3 )
                        TempTimeConstant ( 480 )
                        OptTemperature ( 85 )
                        IdleTemperature ( 42 )
                )
        )

Effects (
		DieselSpecialEffects (
			Exhaust1 ( -0.3 4.6 -0.75
					0 1 0
					0.2
			)
		)
	)
HeadOut ( 1.7 3.25 -4.3 )

ORTSTractionCharacteristics (	10	10												
	throttle (	0	0.06	0.08	0.15	0.27	           0.44	           0.58	            0.81	1.00 )			
	table (													
		0km/h	0.00kN	62.00kN	112.00kN 164.00kN 280.00kN	370.00kN	400.00kN        430.00kN	440.00kN			
		10km/h	0.00kN	14.00kN	30.00kN	 52.00kN 76.00kN	114.00kN	150.00kN	200.00kN	250.00kN			
		20km/h	0.00kN	2.00kN	20.00kN	 32.00kN 40.00kN	60.00kN	        80.00kN 	106.00kN	128.00kN			
		30km/h	0.00kN	0.00kN	10.00kN	 20.00kN 30.00kN	43.00kN		55.00kN		74.00kN		90.00kN			
		40km/h	0.00kN	0.00kN	5.00kN	 15.00kN 21.00kN	33.00kN		45.00kN		55.00kN		68.00kN			
		50km/h	0.00kN	0.00kN	2.00kN	 10.00kN 14.00kN	25.00kN		37.00kN		46.50kN		56.00kN			
		60km/h	0.00kN	0.00kN	0.00kN	 2.00kN 7.00kN 	        18.00kN		31.00kN		39.00kN		47.00kN			
		70km/h	0.00kN	0.00kN	0.00kN 	 0.00kN	2.00kN		12.00kN		25.00kN		34.00kN		39.00kN			
		80km/h	0.00kN	0.00kN	0.00kN	 0.00kN	0.00kN		8.00kN		18.00kN		26.00kN		33.00kN			
		90km/h	0.00kN	0.00kN	0.00kN	 0.00kN	0.00kN		5.00kN		14.00kN		20.00kN		27.00kN			
		)													
	)
comment (** brzdy - brzdove systemy a ovladaci prvky **)

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Blended" )

comment (** kompresor a tlaky v jimkach, vlastnosti potrubi **)

	AirBrakesMainMaxAirPressure ( 9bar )
	AirBrakesCompressorRestartPressure ( 6.8bar )
	AirBrakesMainResVolume ( 1000l )
	comment (** doba plneni hlavni jimky/vykon kompresoru - vypoctena doba plneni 1000l jimky 2.93min.
  	  	kompresor K2lok1, prikon 19.5kW, saci vykon 180m^3/h (dle prirucky 120 - 230m^3/h).
		Vypoctena rychlost plneni jimky 0.742psi/s = 0.0512bar/s**)
	ORTSMainResChargingRate ( 0.0512bar/s )
	ORTSBrakePipeChargingRate ( 4.6bar/s )
	comment (** unik vzduchu netesnostmi brzdoveho potrubi **)
	TrainPipeLeakRate ( 0.00066bar/s )
	ORTSBrakePipeTimeFactor ( 0.003 )
	ORTSBrakeServiceTimeFactor ( 1.009 )
	ORTSBrakeEmergencyTimeFactor ( 0.1 )
comment (** samocinna prubezna brzda - DAKO BS-2 **)

	TrainBrakesControllerMaxSystemPressure ( 5bar )
	TrainBrakesControllerMaxQuickReleaseRate ( 0.625bar/s )
	TrainBrakesControllerMaxReleaseRate ( 0.166bar/s )
	TrainBrakesControllerMaxApplicationRate ( 0.166bar/s )
	TrainBrakesControllerEmergencyApplicationRate ( 0.83bar/s )
	TrainBrakesControllerFullServicePressureDrop ( 2bar )
	TrainBrakesControllerMinPressureReduction ( 0.2bar ) 
comment (** primocinna brzda DAKO BP **)

	EngineBrakesControllerMaxSystemPressure ( 5bar )
	EngineBrakesControllerMaxReleaseRate ( 1.4bar/s )
	EngineBrakesControllerMaxApplicationRate (1.4bar/s )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerEmergencyApplicationRate ( 0.159bar/s )
	EngineBrakesControllerFullServicePressureDrop ( 1.5bar )
	EngineBrakesControllerMinPressureReduction ( 0.2bar )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
  	EngineBrakesControllerHasProportionalBrake ( 1 )
  	EngineBrakesProportionalBrakeLag ( 0 )
	ORTSEngineBrakeApplicationRate ( 1.0bar/s )
	ORTSEngineBrakeReleaseRate ( 2.0bar/s ) 
CabView ( "../../common.cab/cab770_5/770_5.cvf" )

VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 27 )
		MonitoringDeviceAlarmTimeLimit ( 17 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)

EngineControllers (
            Throttle ( 0 1 0.04 0
                NumNotches ( 9
                    Notch ( 0       0 Dummy )
                    Notch ( 0.06    0 Dummy )
                    Notch ( 0.08    0 Dummy )
                    Notch ( 0.15    0 Dummy )
                    Notch ( 0.27    0 Dummy )
                    Notch ( 0.44    0 Dummy )
                    Notch ( 0.58    0 Dummy )
                    Notch ( 0.81    0 Dummy )
                    Notch ( 1       0 Dummy )
			)
		)
		Brake_Engine ( 0 1 0.2 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)            
            comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 7
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.80 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.87 0 TrainBrakesControllerHoldLappedStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		BellToggle( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		Wipers ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
	)
Sound ( "../../common.snd/snd770/770orcab.sms" )
Name ("LRL 620 037-3")
Description (T669)
)