SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( zsskc_751197

	Comment ( Svetla + trakcia OR: Robo )
	Comment ( ORTSDieselEngines: Igor Hnizdo )
	Comment ( GC75P )
	
  Type ( Engine )
 WagonShape ( zsskc_751197.s )
 Freightanim ( zsskc_751197_1.s 1 1 )
 
 Size ( 3.2m 4.46m 15.7m )  
 
 Mass ( 75t )
 WheelRadius ( 0.5m )
 InertiaTensor ( Box ( 3.2m 4.46m 15.7m ) )

Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )

	ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*75t )
	DerailBufferForce ( 350kN )
	NumWheels ( 4 )
	Friction (
		994.0N/m/s    -0.10    1.4mph    12.766N/m/s    1.895
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)

	MaxBrakeForce( 85.19kN )
	MaxHandbrakeForce( 27.90kN )
	NumberOfHandbrakeLeverSteps( 10 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
        BrakeSystemType( "Air_single_pipe" )
        TripleValveRatio( 2.5 )
        MaxReleaseRate( 1.6 )
        MaxApplicationRate( 1.5 )
        MaxAuxilaryChargingRate( 4.28 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 52.50 )
        BrakePipeVolume ( 0.50 )
Comment (** Prubeh soucinitele treni dle rychlosti - litinove brzdove spalky **)

  	  ORTSBrakeShoeFriction (
  			0	0.31
			1	0.30
			2	0.28
			3	0.27
			4	0.26				
			5	0.25
			7	0.24
			8	0.23
			9	0.22
			12	0.21
			14	0.20
			17	0.19
			20	0.18
			24	0.17
			29	0.16
			34	0.15
			40	0.14
			47	0.13
			55	0.12
			66	0.11
			84	0.10
			115	0.09
			160	0.09
	)

 IntakePoint ( 0 1 FuelDiesel )

 	Lights ( 23
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFF9FFFF )
					Position ( 0 3.6 7 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFD2935E )
					Position ( 0 3.6 7 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 20 )
				)
			)
		)
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( Reflektor plny )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFF9FFFF )
					Position ( 0.0 3.656 7.76 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
                 Light (
			comment ( Reflektor tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFD2935E )
					Position ( 0.0 3.656 7.76 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.8 1.389 7.67 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.8 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( Reflektor plny )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFF9FFFF )
					Position ( 0.0 3.656 -7.76 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.8 )
				)
			)
		)
                Light (
			comment ( Reflektor tlmeny )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFD2935E )
					Position ( 0.0 3.656 -7.76 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.8 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.8 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		comment ( Definice svetel pro Loose consist )

		Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.8 1.389 7.67 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.8 1.389 -7.67 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		comment ( Definicia svetel pre posunujuci diel )

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.8 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.8 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.8 1.389 7.67 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC reflektor prední 1 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFD2935E )
					Position ( 0.0 3.656 7.76 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.8 1.389 -7.67 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
 	Sound ( "..//..//common.snd//snd751//751teengII.sms" )
 	
)

Engine ( zsskc_751197
ORTSDieselEngines ( 1
                Diesel (
                        IdleRPM ( 300 )
                        MaxRPM ( 775 )
                        StartingRPM ( 280 )
                        StartingConfirmRPM ( 301 )
                        ChangeUpRPMpS ( 38 )
                        ChangeDownRPMpS ( 26 )
                        RateOfChangeUpRPMpSS ( 100 )
                        RateOfChangeDownRPMpSS ( 100 )
                        MaximalPower ( 980kW )
                        IdleExhaust ( 0.12 )
                        MaxExhaust ( 2.15 )
                        ExhaustDynamics ( 1.6 )
                        ExhaustColor ( 15FF00FF )
                        ExhaustTransientColor ( 90EAf9FF )
                        DieselPowerTab (
                                0  0
                                300  22000
                                306  30000
                                319  60000
				330  120000
				415  280000
				505  455000
				595  630000
				685  805000
				775  980000
                        )
                        DieselConsumptionTab (
                                0  0
                                300  11.0
                                306  19.0
                                319  28.0
				330  43.0
				415  85.0
				505  134.0
				595  185.0
				685  243.0
				775  304.0
                        ) 
                        ThrottleRPMTab (
                                0  300
                                3  306
                                6  319
                                12  330
                                29  415
                                46  505
                                64  595
                                82  685
                                100  775
                        )
                        DieselTorqueTab (
                                0  0
                                300  700.33
                                306  942.43
                                319  1860.39
				330  3472.72
				415  6443.37
				505  8604.46
				595  10111.76
				685  11223.0
				775  12076.12
                        )
                        MinOilPressure ( 36.20 )
                        MaxOilPressure ( 88 )
                        MaxTemperature ( 115 )
                        Cooling ( 3 )
                        TempTimeConstant ( 480 )
                        OptTemperature ( 85 )
                        IdleTemperature ( 42 )
                )
        )
 Effects (
		DieselSpecialEffects (
			Exhaust1
			(
					0.219 4.35 2.143
					0 1 0
					0.2
			)
		)
	)

 Wagon ( zsskc_751197 )
 Type ( Diesel )
	MaxPower ( 980kW ) 
      	MaxForce ( 180kN )
	MaxContinuousForce ( 120kN )
	MaxVelocity ( 100km/h )
	MaxCurrent ( 3500A )
	WheelRadius ( 0.5m )
	Sanding ( 24km/h )
	NumWheels ( 4 )
	DieselEngineType ( electric )
	DieselEngineSpeedOfMaxTractiveEffort( 28km/h )

  CabView ( "../../common.cab/cab751/751zscs2E.cvf" )
      HeadOut ( 1.7 3.2 6.8 )
 MaxDieselLevel ( 2500l )

	AirBrakesAirCompressorPowerRating ( 1.67 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 131 )	
	AirBrakesMainResVolume ( 35.315 )
	AirBrakesAirCompressorWattage ( 20000 )
	AirBrakesCompressorRestartPressure ( 102 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 4.818 )
TrainBrakesControllerMaxApplicationRate ( 1.07 )
TrainBrakesControllerMaxReleaseRate ( 1.07 )
TrainBrakesControllerMaxQuickReleaseRate ( 2.14 )
TrainBrakesControllerEmergencyApplicationRate ( 5 )
TrainBrakesControllerMinSystemPressure ( 3 )
TrainBrakesControllerMaxSystemPressure ( 73 )
TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
TrainBrakesControllerMaxPressureDropInNormalApplication ( 29.2 )
TrainPipeLeakRate ( 0.033 )
TrainBrakesControllerFullServicePressureDrop ( 29.2 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

 DoesHornTriggerBell( 0 )
 
 MaxSandingTime( 800 )
 comment(        320kg )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 27 )
		MonitoringDeviceAlarmTimeLimit ( 17 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 65.1 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)
	
		
 
       EngineControllers (
		Throttle ( 0 1 0.125 0
			NumNotches ( 9
				Notch ( 0    0 Dummy )
				Notch ( 0.03 0 Dummy )
				Notch ( 0.06 0 Dummy )
				Notch ( 0.12 0 Dummy )
				Notch ( 0.29 0 Dummy )
				Notch ( 0.46 0 Dummy )
				Notch ( 0.64 0 Dummy )
				Notch ( 0.82 0 Dummy )
				Notch ( 1    0 Dummy )
			)
		)            
		comment (***Primocinna brzda typ DAKO-BP***)
		Brake_Engine ( 0 1 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )                   
                )
            )
            comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 6
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
            Brake_Hand ( 0 1 0.125 0 
       NumNotches( 1
                    Notch(0    1 Dummy)
                )
            )

            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
	ORTSTractionCharacteristics (	12	10												
	throttle (	0	0.03	0.06	0.12	0.29	           0.46	           0.64	            0.82	1.00 )			
	table (													
		0km/h	0.00kN	30.00kN	77.00kN	128.00kN 180.00kN	180.00kN	180.00kN	180.00kN	180.00kN			
		10km/h	0.00kN	10.00kN	17.00kN	39.00kN	83.00kN	        135.00kN	165.00kN	170.00kN	180.00kN			
		20km/h	0.00kN	5.00kN	10.00kN	18.00kN	46.00kN		73.00kN		100.00kN	127.00kN	150.00kN
                24km/h	0.00kN	4.50kN	8.00kN  15.00kN 37.00kN         60.00kN         83.00kN         103.00kN        129.00kN
      		30km/h	0.00kN	4.00kN	6.00kN	13.00kN	30.00kN		50.00kN		69.00kN 	88.00kN		108.00kN			
		40km/h	0.00kN	3.00kN	5.00kN	10.00kN	23.00kN		38.00kN		52.00kN		67.00kN		81.00kN			
		50km/h	0.00kN	2.00kN	4.00kN	8.50kN	18.00kN		30.00kN		43.00kN		53.00kN		66.00kN			
		60km/h	0.00kN	1.00kN	3.00kN	6.50kN	15.00kN		25.00kN		35.00kN		45.50kN		55.00kN			
		70km/h	0.00kN	0.00kN	2.00kN	5.50kN	13.00kN		22.00kN		30.00kN		38.00kN		47.00kN			
		80km/h	0.00kN	0.00kN	1.00kN	4.50kN	12.00kN		18.00kN		26.00kN		34.00kN		41.00kN			
		90km/h	0.00kN	0.00kN	0.00kN	4.00kN	9.00kN		15.00kN		21.00kN		30.00kN		37.00kN			
		100km/h	0.00kN	0.00kN	0.00kN	3.50kN	7.00kN		10.00kN		17.00kN		24.00kN		33.00kN			
		)													
	)

 comment( fuel_level )
 EngineVariables ( 500 )
  Sound ( "../../common.snd/snd751//751tecabII.sms" )
  Name ( "ZSSKC 751 197-5" )
  Description (
 "Rada 749 CD je univerzalni dieselelektricka skrinova lokomotiva, pouzivana v osobni i nakladni doprave.\n\n"+
 "Lokomotiva je vybavena generatorem 3000V pro vytapeni vlakovych souprav.\n\n"+
 "Prenos vykonu: elektricky\n\n"+
 "Zdroj vykonu: naftovy motor CKD K 6 S 310 DR\n\n"+
 "Max. vykon motoru: 1103 kW\n\n"+
 "Max. trakcni vykon: 990 kW\n\n"+
 "Max. vyska: 4,1 m\n\n"+
 "Max. sirka: 3,1 m\n\n"+
 "Delka pres narazniky: 16,5 m\n\n"+
 "Hmotnost: 72 t\n\n"+
 "Max. rychlost: 100 km/h"
  )
 EngineOperatingProcedures (
 "To move forward\n"+
 "1. Press the W key to move the Reverser to Forward.\n"+
 "2. Press the ; (SEMICOLON) key to release the train brakes.\n"+
 "3. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
 "4. Press the D key to move the throttle from Idle to Notch 1.\n"+  
 "5. Gradually increase power (D key), one notch at a time, until your train reaches the desired speed.\n\n"+
 "To slow the train\n"+
 "1. Press the A key to move the throttle to a lower setting.\n"+
 "2. Use the brakes to further reduce speed if desired.\n\n"+  
 "To apply the dynamic brakes\n"+
 "1. Press the A key to move the throttle to the Idle position.\n"+
 "2. Wait for 10 seconds, then press the . (PERIOD) key to advance the Dynamic Brake handle from Off to the Setup position.  After allowing a few seconds for braking circuit setup, press the . [PERIOD] key again to set the desired level of dynamic braking (Levels 1 - 8).\n\n"+
 "To release the dynamic brakes\n"+
 "1. Press the D key to move the throttle towards Idle.\n\n"+
 "To apply the train brakes\n"+
 "1. Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
 "To bail off the train brakes on the locomotive\n"+
 "1. Press the / (FORWARD SLASH) key.\n\n"+
 "To release the train brakes\n"+
 "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
 "To apply the locomotive brake\n"+
 "1. Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
 "To release the locomotive brake\n"+
 "1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
 "To activate emergency braking\n"+
 "1. Press the A key to reduce the throttle to Idle.\n"+
 "2. Press the BACKSPACE key to activate emergency braking.\n\n"+
 "To back up\n"+
 "1. Bring your train to a full stop.\n"+ 
 "2. Press the S key to move the Reverser to the Reverse position.\n"+
 "4. Release the brakes.\n"+
 "5. Slowly advance the throttle lever (D key).\n\n"+
 "To couple to a car or locomotive\n"+
 "1. Coast into the unit at a very slow speed, about 2 mph.\n"+
 "TIP: To use the Coupling view, press the 6 key.\n"+
 "2. Press F9 to open the Train Operations window.\n"+
 "3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
 "4. Close the Train Operations window.\n\n"+
 "To uncouple from a car or locomotive\n"+
 "1. Press F9 to open the Train Operations window.\n"+
 "2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
 "3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
 "4. Close the Train Operations window."
 ) 

)
