SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( awt_770534rv
	Type ( Engine )
	WagonShape ( awt_770534rv.s )
	Freightanim ( awt_770534freightrv.s 1 1 )

	Comment ( svetla: Robo )
	Commnet ( ladenie OR )
		
Comment	( Overall physics )


	Size ( 3.15m 4.76m 16.44m )
	CentreOfGravity ( 0m 2.3m 0m )
	Mass ( 120t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.15m 4.76m 16.44m) )

Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )

comment	( Adhesion and Friction )

	ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*120t )
	DerailBufferForce ( 800kN )
	NumWheels (	6 )
	Friction (
		1538.8N/m/s    -0.10    1.5mph    17.377N/m/s    1.837
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)

	MaxBrakeForce( 124.35kN )
	MaxHandbrakeForce( 13.95kN )
	NumberOfHandbrakeLeverSteps( 10 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
        BrakeSystemType( "Air_single_pipe" )
        TripleValveRatio( 2.5 )
        MaxReleaseRate( 1.6 )
        MaxApplicationRate( 1.5 )
        MaxAuxilaryChargingRate( 4.28 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 52.50 )
        BrakePipeVolume ( 0.52 )
Comment (** Prubeh soucinitele treni dle rychlosti - litinove brzdove spalky **)

  	  ORTSBrakeShoeFriction (
  			0	0.31
			1	0.30
			2	0.28
			3	0.27
			4	0.26				
			5	0.25
			7	0.24
			8	0.23
			9	0.22
			12	0.21
			14	0.20
			17	0.19
			20	0.18
			24	0.17
			29	0.16
			34	0.15
			40	0.14
			47	0.13
			55	0.12
			66	0.11
			84	0.10
			115	0.09
			160	0.09
	)
	
comment	( EngSound, Freight, Inside, IntakePoint )

	IntakePoint ( 0 2 FuelDiesel )

comment	( Lights )

	Lights ( 25
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFCFE )
					Position ( 0 3.6 7 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)
		
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFCFE )
					Position ( -0.115 4.1 7.42 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFCFE )
					Position ( 0.115 4.1 7.42 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední lave zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFCFE )
					Position ( 0.115 4.1 -7.42 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFCFE )
					Position ( -0.115 4.1 -7.42 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední lave zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )
                Light (
			comment ( Prední lave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní prave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro Loose consist )
                Light	(
			comment( lave přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light	(
			comment( prave zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.597 2.02 7.31 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( -0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80ff0000 )
					Position ( 0.597 2.02 -7.31 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
     Sound ( "../../common.snd/snd771/770.5oreng.sms" )
)

Engine ( awt_770534rv  
ORTSDieselEngines ( 1
                Diesel (
                        IdleRPM ( 350 )
                        MaxRPM ( 750 )
                        StartingRPM ( 320 )
                        StartingConfirmRPM ( 351 )
                        ChangeUpRPMpS ( 38 )
                        ChangeDownRPMpS ( 26 )
                        RateOfChangeUpRPMpSS ( 100 )
                        RateOfChangeDownRPMpSS ( 100 )
                        MaximalPower ( 885kW )
                        IdleExhaust ( 0.12 )
                        MaxExhaust ( 2.15 )
                        ExhaustDynamics ( 1.6 )
                        ExhaustColor ( 15FF00FF )
                        ExhaustTransientColor ( 90EAf9FF )
                        DieselPowerTab (
                                0  0
                                350  30000
                                356  53100
                                380  70800
				420  132800
				460  239000
				510  389400
				560  513300
				660  717000
				750  885000
                        )
                        DieselConsumptionTab (
                                0  0
                                350  30.4
                                460  71.4
				510  103.6
				560  146.4
				660  214.3
				750  269.0
                        ) 
                        ThrottleRPMTab (
                                0  350
                                6  356
                                8  380
                                15  420
                                27  460
                                44  510
                                58  560
                                81  660
                                100  750
                        )
                        DieselTorqueTab (
                                0  0
                                350  818.57
                                356  1424.45
                                380  1779.32
				420  3018.48
				460  4960.81
				510  7291.71
				560  8753.6
				660  10373.33
				750  11269
                        )
                        MinOilPressure ( 36.20 )
                        MaxOilPressure ( 88 )
                        MaxTemperature ( 115 )
                        Cooling ( 3 )
                        TempTimeConstant ( 480 )
                        OptTemperature ( 85 )
                        IdleTemperature ( 42 )
                )
        )
	Wagon ( awt_770534rv )

	
comment	( Basic physical engine data )

	Type ( Diesel )
	MaxPower ( 885kW )
	MaxForce ( 310kN )	
	MaxContinuousForce ( 180kN )
	MaxCurrent ( 2340A ) 
	MaxVelocity ( 90km/h )
	DieselEngineSpeedOfMaxTractiveEffort( 15.5km/h )  
	WheelRadius ( 0.5m )
	comment( sanding system is switched off when faster than given velocity )
	Sanding ( 1e9mph )
	NumWheels ( 6 )
	
	
comment	( CabSound and Views )

	Sound ( "../../common.snd/snd771/771orcab.sms" )

	CabView ( "../../common.cab/cab770_5/770_5okdRV.cvf" )
	
	HeadOut ( 1.7 3.1 4.5 )
	DieselEngineType ( electric )
	MaxDieselLevel ( 1585gal )

comment	( Smoke and Steam )

	Effects (
		DieselSpecialEffects (
			Exhaust1 ( 0.201 4.55 1.756
					0 1 0
					0.1
			)
		)
	)

comment	( Brakes )


	AirBrakesAirCompressorPowerRating ( 1.67 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 131 )	
	AirBrakesMainResVolume ( 35.315 )
	AirBrakesAirCompressorWattage ( 35000 )
	AirBrakesCompressorRestartPressure ( 102 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 4.818 )
TrainBrakesControllerMaxApplicationRate ( 1.07 )
TrainBrakesControllerMaxReleaseRate ( 1.07 )
TrainBrakesControllerMaxQuickReleaseRate ( 2.14 )
TrainBrakesControllerEmergencyApplicationRate ( 5 )
TrainBrakesControllerMinSystemPressure ( 3 )
TrainBrakesControllerMaxSystemPressure ( 73 )
TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
TrainBrakesControllerMaxPressureDropInNormalApplication ( 29.2 )
TrainPipeLeakRate ( 0.033 )
TrainBrakesControllerFullServicePressureDrop ( 29.2 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

comment ( Monitors )

	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 58.9 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 59 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 0 )
	)
EngineVariables( 1200 )

comment	( Controllers )

	EngineControllers (
            Throttle ( 0 1 0.04 0
                NumNotches ( 9
                    Notch ( 0       0 Dummy )
                    Notch ( 0.06    0 Dummy )
                    Notch ( 0.08    0 Dummy )
                    Notch ( 0.15    0 Dummy )
                    Notch ( 0.27    0 Dummy )
                    Notch ( 0.44    0 Dummy )
                    Notch ( 0.58    0 Dummy )
                    Notch ( 0.81    0 Dummy )
                    Notch ( 1       0 Dummy )
			)
		)
		Brake_Engine ( 0 1 0.125 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)            
            comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 6
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
		Brake_Hand ( 0 1 0.0125 0 
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		DirControl ( -1 0 1 1 )
		BellToggle( 0 1 0 )
		AWS ( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		Wipers ( 0 1 0 )
		EmergencyStopToggle ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		BailOffButton( 0 1 0 )
	)
	ORTSTractionCharacteristics (	10	10												
	throttle (	0	0.06	0.08	0.15	0.27	           0.44	           0.58	            0.81	1.00 )			
	table (													
		0km/h	0.00kN	62.00kN	112.00kN 164.00kN 280.00kN	290.00kN	310.00kN	310.00kN	310.00kN			
		10km/h	0.00kN	14.00kN	30.00kN	 52.00kN 76.00kN	114.00kN	150.00kN	200.00kN	250.00kN			
		20km/h	0.00kN	2.00kN	20.00kN	 32.00kN 40.00kN	60.00kN	        80.00kN 	106.00kN	128.00kN			
		30km/h	0.00kN	0.00kN	10.00kN	 20.00kN 30.00kN	43.00kN		55.00kN		74.00kN		90.00kN			
		40km/h	0.00kN	0.00kN	0.00kN	 15.00kN 21.00kN	33.00kN		45.00kN		55.00kN		68.00kN			
		50km/h	0.00kN	0.00kN	0.00kN	 10.00kN 14.00kN	25.00kN		37.00kN		46.50kN		56.00kN			
		60km/h	0.00kN	0.00kN	0.00kN	 2.00kN 7.00kN 	        18.00kN		31.00kN		39.00kN		47.00kN			
		70km/h	0.00kN	0.00kN	0.00kN 	 0.00kN	2.00kN		12.00kN		25.00kN		34.00kN		39.00kN			
		80km/h	0.00kN	0.00kN	0.00kN	 0.00kN	0.00kN		8.00kN		18.00kN		26.00kN		33.00kN			
		90km/h	0.00kN	0.00kN	0.00kN	 0.00kN	0.00kN		5.00kN		14.00kN		20.00kN		27.00kN			
		)													
	)
	
Comment	( Operations )


    	Name ( "AWT 770 534-6 rv" )
    	Description (
		"CME3 je diesel-electrická lokomotiva vyvinutá v roce 1963. Kvuli nedostatecne vyrobni kapacite pokryvajici vyvoz"+
		"do Sovetského svazu byla vyroba pro CSSR zavedena v SMZ Dubnica v roce 1967.\n\n"+
		"Typ lokomotivy: Diesel-Elektrická\n"+
		"Motor: K6S310DR\n"+
		"Výkon motoru: 993 kW\n"+
		"Max. provozní rychlost: 90 km/h\n"+
		"Max. tazná síla na háku: 310 kN\n\n"+
		"Trvalá tazná síla na háku: 188 kN\n\n"+
		"Max. výska: 4.64 m\n\n"+
		"Délka pres nár.: 17.24 m\n\n"+
		"Max. sírka: 3.15 m\n\n"+
		"Hmotnost: 115,8t" 
		"Usporádání dvojkolí: Co'Co'\n\n"+
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
		"4.	Stisknete D pro zvýsení pozadovaného výkonu.\n"+
		"5.	Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jedním stiskem ' presunte vlakovou brzdu do polohy ZÁVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
		"Jak pouzít vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
		"2.	Po dosazení pozadovaného brzdného tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
		"2.	Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
		"3.	Po odbrzdení a uvedení vlaku do pohybu stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n\n"+
 		"Jak pouzít lokomotvní brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivní brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0%).\n\n"+
		"Jak pouzít záchrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snízení výkonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
		"Jak zrusit záchrannou brzdu\n"+
		"1.	Pockejte na úplné zastavení vlaku.\n"+
		"2.	Stisknete Z pro odblokování ovládání lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
		"4.	Pomalu zvysujte výkon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Výstup a nástup cestujících\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahájení výstupu a nástupu cestujících.\n"+
		"3.	Pockejte na signál k odjezdu.\n"+
		"TIP: Pro zobrazení casu príjezdu a odjezdu u této a následující stanice pouzijte klávesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimální rychlost 1 km/h).\n"+
		"Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
		"2.	Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdíte pripojené vozy.\n\n"+
		"Odpojení vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftového stojanu stredem nádrze.\n"+
		"2.	Stisknete klávesu T a drzte ji po dobu doplnování nafty stisknutou.\n"+
		"TIP: Pro zobrazení prubehu plnení nádrze stisknete F9 a klepnete mysí na ikonu lokomotivy.\n\n"+
	)
)
