SIMISA@@@@@@@@@@JINX0D0t______
 
Wagon ( zsr_781312
 
        Comment ( ladenie OR )
        Comment ( svetla Robo )
 
 Type ( Engine )
 WagonShape ( zsr_781312.s )
 Freightanim ( zsr_781312fg.s 1 1 )
 Size ( 3.44m 4.68m 17.01m )  
 Mass ( 116.5t )
 WheelRadius ( 0.525m ) 
 InertiaTensor ( Box ( 3.44m 4.68m 17.01m ) )
  
Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 7.5e6N/m 1e7N/m )
   Damping ( 1e6N/m/s 2e6N/m/s )
   Break ( 1.1e8N 5e8N )
   r0 ( 80cm 150cm )
  )
  CouplingHasRigidConnection ( 0 )
  Velocity ( 0.01m/s )
 )

 ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        )
 DerailRailHeight ( 10cm )
 DerailRailForce ( 2.5*116.5t )
 DerailBufferForce ( 2000kN )
 NumWheels ( 6 )

Friction (
		1516.5N/m/s    -0.10    1.4mph    16.379N/m/s    1.867
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)


	MaxBrakeForce( 130.01kN )
	MaxHandbrakeForce( 27.90kN )
	NumberOfHandbrakeLeverSteps( 10 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
        BrakeSystemType( "Air_single_pipe" )
        TripleValveRatio( 2.5 )
        MaxReleaseRate( 1.6 )
        MaxApplicationRate( 1.5 )
        MaxAuxilaryChargingRate( 4.28 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 52.50 )
        BrakePipeVolume ( 0.53 )
Comment (** Prubeh soucinitele treni dle rychlosti - litinove brzdove spalky **)

  	  ORTSBrakeShoeFriction (
  			0	0.31
			1	0.30
			2	0.28
			3	0.27
			4	0.26				
			5	0.25
			7	0.24
			8	0.23
			9	0.22
			12	0.21
			14	0.20
			17	0.19
			20	0.18
			24	0.17
			29	0.16
			34	0.15
			40	0.14
			47	0.13
			55	0.12
			66	0.11
			84	0.10
			115	0.09
			160	0.09
	)

 IntakePoint ( 0 1 FuelDiesel )

comment	( Lights )

	Lights ( 23
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFFFF )
					Position ( 0 3.6 7 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 60 )
				)
			)
		)
		Light (
			comment ( Svetelný kuzel tlumený )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0 3.6 7 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 20 )
				)
			)
		)
		comment ( Definice svetel pro prední stanoviste )

		Light (
			comment ( reflektor dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFFFF )
					Position ( 0.0 4.14 8.1 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 1.8 )
				)
			)
		)
		Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0.0 4.14 8.1 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -1.07 1.56 8.15 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 1.07 1.56 8.15 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.30 1.56 -8.15 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.30 1.56 -8.15 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor dálkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFFFF )
					Position ( 0.0 4.14 -8.1 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 1.8 )
				)
			)
		)
		Light (
			comment ( reflektor tlumený )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0.0 4.14 -8.1 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.8 )
				)
			)
		)
		Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 1.07 1.56 -8.15 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -1.07 1.56 -8.15 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.30 1.51 8.1 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.30 1.51 8.1 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
        comment ( Definice svetiel pre LC )

		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 1.07 1.56 8.15 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -1.07 1.56 -8.15 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
        comment ( Definice svetiel pre posunujuci diel )

		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.0 )
			FadeOut ( 0.0 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 1.07 1.56 8.15 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.3 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -1.07 1.56 -8.15 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( 1.07 1.56 8.15 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBDEBE )
					Position ( -1.07 1.56 8.15 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC reflektor prední )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEBBF9C )
					Position ( 0.0 4.14 8.1 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 1.2 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.30 1.51 -8.1 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.30 1.51 -8.1 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
 Sound ( "../../common.snd/snd781/781eng.sms" )
)

Engine ( zsr_781312
ORTSDieselEngines ( 1
                Diesel (
                        IdleRPM ( 400 )
                        MaxRPM ( 770 )
                        StartingRPM ( 380 )
                        StartingConfirmRPM ( 401 )
                        ChangeUpRPMpS ( 38 )
                        ChangeDownRPMpS ( 26 )
                        RateOfChangeUpRPMpSS ( 100 )
                        RateOfChangeDownRPMpSS ( 100 )
                        MaximalPower ( 1232kW )
                        IdleExhaust ( 0.12 )
                        MaxExhaust ( 2.15 )
                        ExhaustDynamics ( 1.6 )
                        ExhaustColor ( 15FF00FF )
                        ExhaustTransientColor ( 90EAf9FF )
                        DieselPowerTab (
                                0  0
                                400  45000
                                406  50000
                                425  150000
				450  200000
				475  400000
                                500  450000
                                525  500000
				550  550000
				575  650000
				600  700000
				625  750000
                                650  800000
				675  900000
				700  1000000
				725  1100000
				750  1232000
			)
                        DieselConsumptionTab (
                                0  0
                                400  35.2
                                500  150.0
                                550  173.8
				600  204.8
				625  223.8
				650  242.9
				675  273.8
				700  304.8
				725  354.0
                                750  408.0
                        ) 
                        ThrottleRPMTab (
                                0    400
                                4.1  406
                                12.2 425
                                16.2 450
                                32.5 475
                                36.5 500
                                40.6 525
                                44.6 550
                                52.8 575
                                56.8 600
                                60.9 625
                                64.9 650
                                73.1 675
                                82.2 700
                                89.3 725
                               100   750
                        )
                        DieselTorqueTab (
                                0  0
                                400  1074.38
                                406  1193.75
                                425  3370.59
				450  4244.44
				475  8042.11
				500  8595
				525  9095.24
				550  9550
				575  10795.65
                                600  11460
				625  11753.85
				650  12733.33
				675  13642.86
				700  13642.86
                                725  14489.66
                                750  15687.47
                        )
                        MinOilPressure ( 36.20 )
                        MaxOilPressure ( 88 )
                        MaxTemperature ( 115 )
                        Cooling ( 3 )
                        TempTimeConstant ( 480 )
                        OptTemperature ( 85 )
                        IdleTemperature ( 42 )
                )
        )
 Effects
 (
  DieselSpecialEffects
  (
   Exhaust1
			(
                                0.0 4.52 2.6
				0 0.2 0
				0.3			
				
			)
  )
 )        

 Wagon ( zsr_781312 )
 Type ( Diesel )
 MaxPower ( 1232kW )
 MaxForce ( 370kN ) 
 MaxContinuousForce ( 190kN ) 
 MaxVelocity ( 100km/h )
 MaxCurrent ( 8919A )
 DieselEngineSpeedOfMaxTractiveEffort( 22km/h ) 
 HeadOut ( 1.72 3.3 6.8 )
 WheelRadius ( 0.525m ) 
 Vigilance ( 1 )
 Sanding ( 1e9mph )
 NumWheels ( 6 )

	AirBrakesAirCompressorPowerRating ( 1.67 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 131 )	
	AirBrakesMainResVolume ( 46.898 )
	AirBrakesAirCompressorWattage ( 20000 )
	AirBrakesCompressorRestartPressure ( 114 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 4.818 )
TrainBrakesControllerMaxApplicationRate ( 1.07 )
TrainBrakesControllerMaxReleaseRate ( 1.07 )
TrainBrakesControllerMaxQuickReleaseRate ( 2.14 )
TrainBrakesControllerEmergencyApplicationRate ( 5 )
TrainBrakesControllerMinSystemPressure ( 3 )
TrainBrakesControllerMaxSystemPressure ( 73 )
TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
TrainBrakesControllerMaxPressureDropInNormalApplication ( 29.2 )
TrainPipeLeakRate ( 0.033 )
TrainBrakesControllerFullServicePressureDrop ( 29.2 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )
 
 CabView ( "../../common.cab/cab781/781_I.cvf" )
 MaxDieselLevel ( 3900l )

 DoesHornTriggerBell( 0 ) 
 
 MaxSandingTime( -1 )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 27 )
		MonitoringDeviceAlarmTimeLimit ( 17 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 90 )
		MonitoringDeviceCriticalLevel ( 65.1 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 65.2 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)


        EngineControllers (
            Throttle ( 0 1 0.2 0 
                NumNotches ( 16
                    Notch ( 0       0 Dummy )
                    Notch ( 0.041   0 Dummy )
                    Notch ( 0.122   0 Dummy )
                    Notch ( 0.162   0 Dummy )
                    Notch ( 0.325   0 Dummy )
                    Notch ( 0.365   0 Dummy )
                    Notch ( 0.406   0 Dummy )
                    Notch ( 0.446   0 Dummy )
                    Notch ( 0.528   0 Dummy )
                    Notch ( 0.568   0 Dummy )
                    Notch ( 0.609   0 Dummy )
                    Notch ( 0.649   0 Dummy )
                    Notch ( 0.731   0 Dummy )
                    Notch ( 0.812   0 Dummy )
                    Notch ( 0.893   0 Dummy )
                    Notch ( 1       0 Dummy )
                )
            )
            Brake_Engine ( 0 1 0.05 0 
                NumNotches ( 1
                    Notch ( 0       1 Dummy )                    
                )
            )
            comment (***Prubezna brzda typ DAKO-BS2***)
		Brake_Train ( 0 1 0.04 0.87
			NumNotches ( 6
				Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
				Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
				Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
				Notch ( 0.99 0 TrainBrakesControllerEmergencyStart )
			)
		)
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            )
	ORTSTractionCharacteristics (	11	17												
	throttle (	0	0.06	0.14	0.18	 0.34	  0.38	   0.42	         0.46	0.54	           0.58	           0.62         0.66               0.74            0.82	            0.91	1.00 )			
	table (													
		0km/h	0.00kN	40.00kN	80.00kN	100.00kN 170.00kN 191.00kN 202.00kN	217.00kN 233.00kN	254.00kN	270.00kN	300.00kN	330.00kN	360.00kN	370.00kN	370.00kN			
		10km/h	0.00kN	30.00kN	40.00kN	60.00kN	110.00kN 123.00kN 137.00kN	150.00kN 163.00kN       179.00kN	195.00kN	209.00kN	223.00kN	240.00kN	250.00kN	260.00kN			
		20km/h	0.00kN	20.00kN	30.00kN	40.00kN	63.00kN	75.00kN	 84.00kN	93.00kN	 103.00kN	113.00kN	126.00kN	136.00kN	150.00kN	165.00kN	180.00kN	194.00kN			
		30km/h	0.00kN	10.00kN	20.00kN	32.00kN	43.00kN	48.00kN	 52.00kN        57.00kN	 62.00kN	67.00kN		74.00kN		82.00kN		96.00kN		110.00kN 	124.00kN	135.00kN			
		40km/h	0.00kN	0.00kN	10.00kN	24.00kN	28.00kN	33.00kN	 38.00kN        41.00kN	 45.00kN	49.00kN		55.00kN		61.00kN		69.00kN		77.00kN		87.00kN		96.00kN			
		50km/h	0.00kN	0.00kN	0.00kN	18.00kN	23.00kN	26.00kN	 29.00kN        32.00kN	 36.00kN	39.00kN		43.00kN		47.00kN		54.00kN		61.00kN		70.00kN		78.00kN			
		60km/h	0.00kN	0.00kN	0.00kN	12.00kN	15.00kN	18.00kN	 22.00kN        25.00kN	 28.00kN	31.00kN		35.00kN		38.00kN		43.00kN		48.00kN		56.50kN		64.00kN			
		70km/h	0.00kN	0.00kN	0.00kN	7.00kN	9.00kN	13.00kN	 15.00kN        18.00kN	 22.00kN	24.00kN		27.00kN		30.00kN		35.00kN		39.00kN		47.00kN		53.00kN			
		80km/h	0.00kN	0.00kN	0.00kN	0.00kN	5.00kN	6.00kN	 9.00kN	        12.50kN	 15.00kN	17.00kN		21.00kN		24.00kN		28.00kN		32.00kN		38.00kN		44.00kN			
		90km/h	0.00kN	0.00kN	0.00kN	0.00kN	0.00kN	1.00kN	 3.00kN	        6.00kN	 9.00kN		12.00kN		15.00kN		18.00kN		22.00kN		26.00kN		32.00kN		37.00kN			
		100km/h	0.00kN	0.00kN	0.00kN	0.00kN	0.00kN	0.00kN	 0.00kN	        3.50kN	 5.00kN		7.00kN		9.00kN		13.00kN		16.00kN		20.00kN		26.00kN		32.00kN			
		)													
	)

 comment( fuel_level )
 EngineVariables ( 3900 )
  Sound ( "../../common.snd/snd781/781cab.sms" )
  Name ( "ZSR 781 312-4" )
  Description (
 "The CD 781 is a Diesel-Electric freight locomotive.\n\n"+
 "Author: HFL.\n"+
 "http://www.ms-trainsimulator.hu\n\n"+
 "Locomotive type: Diesel-Electric\n\n"+
 "Diesel Engine Power: 2000 hp (1472 kW)\n\n"+
 "Real Power: 1160 kW \n\n"+
 "Max. speed: 100 km/h (60 mph)\n\n"+
 "Power source: Kolomna 12 Cylinder Turbocharged Diesel engine\n\n"+
 "Wheel configuration: Six axles, 1050 mm diameter wheels in Co-Co configuration\n\n"+
 "Height: 4.493 m\n\n"+
 "Width: 2.95 m\n\n"+
 "Length: 17.55 m\n\n"+
 "Weight: 116.5 metric tons" 
  )
 EngineOperatingProcedures (
 "To move forward\n"+
 "1. Press the W key to move the Reverser to Forward.\n"+
 "2. Press the ; (SEMICOLON) key to release the train brakes.\n"+
 "3. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
 "4. Press the D key to move the throttle from Idle to Notch 1.\n"+  
 "5. Gradually increase power (D key), one notch at a time, until your train reaches the desired speed.\n\n"+
 "To slow the train\n"+
 "1. Press the A key to move the throttle to a lower setting.\n"+
 "2. Use the brakes to further reduce speed if desired.\n\n"+  
 "To apply the dynamic brakes\n"+
 "1. Press the A key to move the throttle to the Idle position.\n"+
 "2. Wait for 10 seconds, then press the . (PERIOD) key to advance the Dynamic Brake handle from Off to the Setup position.  After allowing a few seconds for braking circuit setup, press the . [PERIOD] key again to set the desired level of dynamic braking (Levels 1 - 8).\n\n"+
 "To release the dynamic brakes\n"+
 "1. Press the D key to move the throttle towards Idle.\n\n"+
 "To apply the train brakes\n"+
 "1. Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
 "To bail off the train brakes on the locomotive\n"+
 "1. Press the / (FORWARD SLASH) key.\n\n"+
 "To release the train brakes\n"+
 "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
 "To apply the locomotive brake\n"+
 "1. Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
 "To release the locomotive brake\n"+
 "1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
 "To activate emergency braking\n"+
 "1. Press the A key to reduce the throttle to Idle.\n"+
 "2. Press the BACKSPACE key to activate emergency braking.\n\n"+
 "To back up\n"+
 "1. Bring your train to a full stop.\n"+ 
 "2. Press the S key to move the Reverser to the Reverse position.\n"+
 "4. Release the brakes.\n"+
 "5. Slowly advance the throttle lever (D key).\n\n"+
 "To couple to a car or locomotive\n"+
 "1. Coast into the unit at a very slow speed, about 2 mph.\n"+
 "TIP: To use the Coupling view, press the 6 key.\n"+
 "2. Press F9 to open the Train Operations window.\n"+
 "3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
 "4. Close the Train Operations window.\n\n"+
 "To uncouple from a car or locomotive\n"+
 "1. Press F9 to open the Train Operations window.\n"+
 "2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
 "3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
 "4. Close the Train Operations window."
 ) 

)
